# Slot 4 Menu 23 − EtherNet/IP Fault Values

Mode: Open‑Loop

Parameter | 4.23.001 Output fault value 1
--- | ---
Short description | Sets the output fault value for mapping 1
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.002 Output fault value 2
--- | ---
Short description | Sets the output fault value for mapping 2
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.003 Output fault value 3
--- | ---
Short description | Sets the output fault value for mapping 3
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.004 Output fault value 4
--- | ---
Short description | Sets the output fault value for mapping 4
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.005 Output fault value 5
--- | ---
Short description | Sets the output fault value for mapping 5
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.006 Output fault value 6
--- | ---
Short description | Sets the output fault value for mapping 6
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.007 Output fault value 7
--- | ---
Short description | Sets the output fault value for mapping 7
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.008 Output fault value 8
--- | ---
Short description | Sets the output fault value for mapping 8
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.009 Output fault value 9
--- | ---
Short description | Sets the output fault value for mapping 9
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.010 Output fault value 10
--- | ---
Short description | Sets the output fault value for mapping 10
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.011 Output fault value 11
--- | ---
Short description | Sets the output fault value for mapping 11
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.012 Output fault value 12
--- | ---
Short description | Sets the output fault value for mapping 12
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.013 Output fault value 13
--- | ---
Short description | Sets the output fault value for mapping 13
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.014 Output fault value 14
--- | ---
Short description | Sets the output fault value for mapping 14
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.015 Output fault value 15
--- | ---
Short description | Sets the output fault value for mapping 15
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.016 Output fault value 16
--- | ---
Short description | Sets the output fault value for mapping 16
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.017 Output fault value 17
--- | ---
Short description | Sets the output fault value for mapping 17
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.018 Output fault value 18
--- | ---
Short description | Sets the output fault value for mapping 18
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.019 Output fault value 19
--- | ---
Short description | Sets the output fault value for mapping 19
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.020 Output fault value 20
--- | ---
Short description | Sets the output fault value for mapping 20
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.021 Output fault value 21
--- | ---
Short description | Sets the output fault value for mapping 21
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.022 Output fault value 22
--- | ---
Short description | Sets the output fault value for mapping 22
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.023 Output fault value 23
--- | ---
Short description | Sets the output fault value for mapping 23
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.024 Output fault value 24
--- | ---
Short description | Sets the output fault value for mapping 24
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.025 Output fault value 25
--- | ---
Short description | Sets the output fault value for mapping 25
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.026 Output fault value 26
--- | ---
Short description | Sets the output fault value for mapping 26
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.027 Output fault value 27
--- | ---
Short description | Sets the output fault value for mapping 27
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.028 Output fault value 28
--- | ---
Short description | Sets the output fault value for mapping 28
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.029 Output fault value 29
--- | ---
Short description | Sets the output fault value for mapping 29
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.030 Output fault value 30
--- | ---
Short description | Sets the output fault value for mapping 30
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.031 Output fault value 31
--- | ---
Short description | Sets the output fault value for mapping 31
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).

Parameter | 4.23.032 Output fault value 32
--- | ---
Short description | Sets the output fault value for mapping 32
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Module reset, EtherNet/IP interface reset or EtherNet/IP interface enable
Display Format | Standard | Decimal Places | 0
Coding | RW, PT

This parameter defines the value to be sent to the mapped output destination when fault values have been configured to be sent (with RPI timeout action (4.20.011) and PLC idle action (4.20.015)).