# Menu 5 Single Line Descriptions − Regen Status

Mode: Regeneration

Parameter | Range | Default | Type
--- | --- | --- | ---
05.001 | Output Frequency | ±200.0 Hz |  | RO | Num | ND | NC | PT | FI
05.002 | Output Voltage | ±VM_AC_VOLTAGE V |  | RO | Num | ND | NC | PT | FI
05.003 | Output Power | ±VM_POWER kW |  | RO | Num | ND | NC | PT | FI
05.005 | D.c. Bus Voltage | ±VM_DC_VOLTAGE V |  | RO | Num | ND | NC | PT | FI
05.007 | Rated Current | ±VM_RATED_CURRENT A | 0.000 A | RW | Num |  | RA |  | US
05.018 | Maximum Switching Frequency | 0 to VM_SWITCHING_FREQUENCY kHz | 3 (1) kHz | RW | Txt |  | RA |  | US
05.023 | D.c. Bus Voltage High Range | ±VM_HIGH_DC_VOLTAGE V |  | RO | Num | ND | NC | PT | FI
05.035 | Auto‑switching Frequency Change | Enabled (0), Disabled (1), No Ripple Detect (2) | Enabled (0) | RW | Txt |  |  |  | US
05.036 | Auto‑switching Frequency Step Size | 1 to 2 | 2 | RW | Num |  |  |  | US
05.037 | Switching Frequency | 2 (0), 3 (1), 4 (2), 6 (3), 8 (4), 12 (5), 16 (6) kHz |  | RO | Txt | ND | NC | PT |
05.038 | Minimum Switching Frequency | 0 to VM_MIN_SWITCHING_FREQUENCY kHz | 3 (1) kHz | RW | Txt |  |  |  | US
05.039 | Maximum Inverter Temperature Ripple | 20 to 60 °C | 60 °C | RW | Num |  |  |  | US

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |