# Slot 4 Menu 11 Single Line Descriptions − Synchronisation

Mode: Open‑Loop

Parameter | Range | Default | Type
--- | --- | --- | ---
4.11.001 | Preferred Sync Master | 0 to 4 | 1 | RW | Num |  |  |  | US
4.11.002 | Master Clock Domain | 0 to 3 | 0 | RW | Num |  |  |  | US
4.11.005 | Grandmaster MAC Address | 00:00:00:00:00:00 to FF:FF:FF:FF:FF:FF |  | RO | Mac | ND | NC | PT |
4.11.006 | Synchronisation Jitter From Grandmaster | -2147483648 to 2147483647 ns |  | RO | Num | ND | NC | PT |
4.11.007 | Synchronisation Jitter Threshold | 500 to 1000000 ns | 1000 ns | RW | Num |  |  |  | US
4.11.008 | Module Synchronised Flag | Off (0) or On (1) | Off (0) | RO | Bit |  |  |  |
4.11.009 | Inhibit Drive Synchronisation | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
4.11.010 | PTP Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT |
4.11.011 | PTP Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT |
4.11.015 | PTP Delay Measurement Select | P2P DELAY (1), OFF (2) | P2P DELAY (1) | RW | Txt |  |  |  | US
4.11.016 | PTP Sync Rate | -4 to 0 | -4 | RW | Num |  |  |  | US
4.11.017 | In sync window length | 3 to 255 s | 20 s | RW | Num |  |  |  | US
4.11.020 | Network Error Count | 0 to 4294967295 |  | RO | Num | ND | NC | PT |
4.11.022 | Interoption Sync Status | MASTER (0), PRODUCER (1), INDEPENDENT (2) |  | RO | Txt | ND | NC | PT |
4.11.030 | Easy Mode Maximum Network Delay | 1 to 100 ms | 3 ms | RW | Num |  |  |  | US
4.11.040 | Rx1 Late Synchronisation Frame Action | Trip (1), Do not use (2), Use (3) | Trip (1) | RW | Txt |  |  |  | US
4.11.041 | Rx1 Late Synchronisation Frame Destination | This slot (0), Slot 1 (1), Slot 2 (2), Slot 3 (3), Slot 4 (4) | This slot (0) | RW | Txt |  |  |  | US
4.11.042 | Rx1 Late Synchronisation Frame Event | No Event (0), Event (1), Event1 (2), Event2 (3), Event3 (4) | No Event (0) | RW | Txt |  |  |  | US
4.11.050 | Rx2 Late Synchronisation Frame Action | Trip (1), Do not use (2), Use (3) | Trip (1) | RW | Txt |  |  |  | US
4.11.051 | Rx2 Late Synchronisation Frame Destination | This slot (0), Slot 1 (1), Slot 2 (2), Slot 3 (3), Slot 4 (4) | This slot (0) | RW | Txt |  |  |  | US
4.11.052 | Rx2 Late Synchronisation Frame Event | No Event (0), Event (1), Event1 (2), Event2 (3), Event3 (4) | No Event (0) | RW | Txt |  |  |  | US
4.11.060 | Rx3 Late Synchronisation Frame Action | Trip (1), Do not use (2), Use (3) | Trip (1) | RW | Txt |  |  |  | US
4.11.061 | Rx3 Late Synchronisation Frame Destination | This slot (0), Slot 1 (1), Slot 2 (2), Slot 3 (3), Slot 4 (4) | This slot (0) | RW | Txt |  |  |  | US
4.11.062 | Rx3 Late Synchronisation Frame Event | No Event (0), Event (1), Event1 (2), Event2 (3), Event3 (4) | No Event (0) | RW | Txt |  |  |  | US

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |