# Menu 3 − Frequency Slaving and Position Feedback

Mode: Open‑Loop

Position feedback interfaces

Two position feedback interfaces with associated freeze system are provided. Access to both these interfaces and the encoder simulation output are provided via one 15 way high density connector. There are limitations on the functions that can be provided simultaneously as shown in the table below along with the connections required for each combination of functions.

Functions | Connections
P1 Position feedback interface | P2 Position feedback interface | Encoder Simulation Output | 1/2 | 3/4 | 5/6 | 7/8 | 9/10 | 11/12 | 13/14 | 15
AB Servo FD Servo FR Servo |  |  | A1 | B1 | Z1 | U1 | V1 | W1 | PS1 | Th
SC Servo |  |  | Cos1 | Sin1 | Z1 | U1 | V1 | W1 | PS1 | Th
AB, FD, FR | AB, FD, FR |  | A1 | B1 | Z1 | A2 | B2 | Z2 | PS1 | Th
AB, FD, FR | EnDat, BiSS, SSI |  | A1 | B1 | Z1 | D2 | Clk2 | Z2 | PS1 | Th
AB, FD, FR |  | Full | A1 | B1 | Z1 | AOut | BOut | ZOut | PS1 | Th
SC | AB, FD, FR |  | Cos1 | Sin1 | Z1 | A2 | B2 | Z2 | PS1 | Th
SC | EnDat, BiSS, SSI |  | Cos1 | Sin1 | Z1 | D2 | Clk2 | Z2 | PS1 | Th
SC |  | Full | Cos1 | Sin1 | Z1 | AOut | BOut | ZOut | PS1 | Th
Resolver | AB, FD, FR |  | Cos1 | Sin1 | Ref1 | A2 | B2 | Z2 | PS1 | Th
Resolver | EnDat, BiSS, SSI |  | Cos1 | Sin1 | Ref1 | D2 | Clk2 | Z2 | PS1 | Th
Resolver |  | Full | Cos1 | Sin1 | Ref1 | AOut | BOut | ZOut | PS1 | Th
SC Hiperface | AB, FD, FR |  | Cos1 | Sin1 | D1 | A2 | B2 | Z2 | PS1 | Th
SC Hiperface | EnDat, BiSS, SSI |  | Cos1 | Sin1 | D1 | D2 | Clk2 | Z2 | PS1 | Th
SC Hiperface |  | Full | Cos1 | Sin1 | D1 | AOut | BOut | ZOut | PS1 | Th
SC EnDat, SC SSI, SC BiSS | AB, FD, FR No Z marker pulse |  | Cos1 | Sin1 | D1 | A2 | B2 | Clk1 | PS1 | Th
SC EnDat, SC SSI, SC BiSS | EnDat, BiSS, SSI |  | Cos1 | Sin1 | D1 | D2 | Clk2 | Clk1 | PS1 | Th
SC EnDat, SC SSI, SC BiSS |  | No Z marker pulse | Cos1 | Sin1 | D1 | AOut | BOut | Clk1 | PS1 | Th
EnDat, BiSS, SSI | AB, FD, FR |  | D1 | Clk1 | Z1 | A2 | B2 | Z2 | PS1 | Th
EnDat, BiSS, SSI | EnDat, BiSS, SSI |  | D1 | Clk1 | Z1 | D2 | Clk2 | Z2 | PS1 | Th
EnDat, BiSS, SSI |  | Full | D1 | Clk1 | Z1 | AOut | BOut | ZOut | PS1 | Th
EnDat, BiSS, SSI | EnDat, BiSS, SSI | No Z marker pulse | D1 | Clk1 | D2 | AOut | BOut | Clk2 | PS1 | Th
SC SC |  |  | Cos1 | Sin1 | Z1 | SCs1 | SSn1 | Z2 | PS1 | Th
Commutation Only |  |  |  |  |  | U1 | V1 | W1 | PS1 | Th
Option Slot 1, 2, 3 or 4 | AB, FD, FR |  |  |  | Z1 | A2 | B2 | Z2 | PS1 | Th
Option Slot 1, 2, 3 or 4 | EnDat, BiSS, SSI |  |  |  | Z1 | D2 | Clk2 | Z2 | PS1 | Th
Option Slot 1, 2, 3 or 4 |  | Full |  |  | Z1 | AOut | BOut | ZOut | PS1 | Th

The marker inputs can be used without their associated position feedback as freeze trigger inputs, therefore these are present where possible even if the associated incremental or SINCOS position feedback is not possible. The table below gives the connection functions associated with the codes used.

Connection Function | Connection Definition
Position Interface inputs
A | A input for AB, or AB Servo encoders F input for FD, FD Servo, FR or FR Servo encoders
B | B input for AB, or AB Servo encoders D input for FD or FD Servo encoders R input for FR or FR Servo encoders
Z | Z input for AB, AB Servo, FD, FD Servo, FR, FR Servo, SC encoders Freeze input
U, V, W | Commutation signals for AB Servo, FD Servo, FR Servo, SC Servo or Commutation Only encoders
Cos, Sin | Cosine and Sine inputs for SC, SC EnDat, SC BiSS, SC Hiperface, SC SSI or SC Servo encoders Cosine and Sine inputs for resolvers
Ref | Reference output for resolvers
D | Data input/output for SC EnDat, SC BiSS, SC Hiperface, EnDat or BiSS encoders Data input for SC SSI, SSI encoders
Clk | Clock output for SC EnDat, SC SSI, EnDat, BiSS or SSI encoders
SCs, SSn | Single turn Cosine and Sine signals used to determine the absolute position within one turn
Encoder Simulation Output
AOut | A output for AB or AB Lock modes F output for FD, FD Lock or FR modes Data output for SSI Gray or SSI Binary modes
BOut | B output for AB or AB Lock modes D output for FD, FD Lock or FR modes Clock input for SSI Gray or SSI Binary modes
Zout | Z output for AB, AB Lock, FD, FD Lock or FR modes
Power Supply and Temperature Measurement
PS1 | Power supply output (13 = Supply, 14 = 0V)
Th | Temperature measurement input

P1 Position feedback interface

P2 Position feedback interface

The P2 position feedback interface duplicates most of the parameter structure and functions of the P1 feedback interface. The P2 interface parameters (03.127 to 03.169) have the same functions as the P1 interface parameters (03.027 to 03.069) except that parameters 03.136, 03.139, 03.162 and 03.163 are not included because the P2 interface does not have its own position feedback power supply, does not support resolvers, and the termination resistors are not selectable and are always enabled. Also P2 Device type (03.138) has less possible settings because the P2 interface does not support all the devices supported by the P1 interface.

Priority of the 15-way D-type is assigned in the following order from the highest priority to the lowest.

1. P1 position interface
2. Encoder simulation output
3. P2 position interface

The availability of the P2 position interface on the 15-way D-type on the drive is dependent on type of feedback device selected in P1 Device Type (03.038) and the encoder simulation mode selected in Encoder Simulation Mode (03.088). P2 Status (03.172) shows the status of the P2 position interface depending on the settings in P2 Device type (03.138), P1 Device Type (03.038), and Encoder Simulation Mode (03.088).

Position feedback initialisation

Position feedback devices need to be initialised before they can provide position feedback information. For details of the initialisation required for each type of device see Position Feedback Initialized (03.076). The user can force all position feedback devices connected directly to the drive or to an option module to be initialised (see Initialise Position Feedback (03.075)). The drive also automatically initialises all position feedback devices connected to the drive position feedback interfaces immediately after power-up. An attempt is made to initialise any position feedback device that needs to be initialised when a drive reset occurs. This would happen inherently if the drive is tripped and the drive is reset to clear the trip.

It should be noted that the initialised bit for any position feedback interface in Position Feedback Initialized (03.076) is set to zero if any of the parameters given below are changed if they could be used by the position feedback device whether rotary or linear. If the parameter could not be used by the device then it remains initialised when the parameter is changed. The initialisation bit for a position feedback device is also set to zero if the number of motor poles parameter for the active motor is changed. If the device becomes uninitialised because of a parameter change then an Encoder 7 trip will occur.

P1 Position feedback interface | P2 Position feedback interface
P1 Rotary Turns Bits (03.033) | P2 Rotary Turns Bits (03.133)
P1 Rotary Lines Per Revolution (03.034) | P2 Rotary Lines Per Revolution (03.134)
P1 Comms Bits (03.035) | P2 Comms Bits (03.135)
P1 Comms Baud Rate (03.037) | P2 Comms Baud Rate (03.137)
P1 Device Type (03.038) |
P1 Auto-configuration Select (03.041) | P2 Auto-configuration Select (03.141)
P1 SSI Incremental Mode (03.047) | P2 SSI Incremental Mode (03.147)
P1 SSI Binary Mode (03.048) | P2 SSI Binary Mode (03.148)
P1 Linear Feedback Select (03.051) | P2 Linear Feedback Select (03.151)
P1 Linear Comms Pitch (03.052) | P2 Linear Comms Pitch (03.152)
P1 Linear Line Pitch (03.053) | P2 Linear Line Pitch (03.153)
P1 Pole Pitch (03.055) | P2 Pole Pitch (03.155)
P1 Feedback Reverse (03.056) | P2 Feedback Reverse (03.156)
P1 Calculation Time (03.060) | P2 Calculation Time (03.160)
P1 Recovery Time (03.061) | P2 Recovery Time (03.161)
P1 Resolver Poles (03.065) |
P1 Resolver Excitation (03.066) |
P1 User Comms Enable (03.067) (EnDat 2.2 only) | P2 User Comms Enable (03.167) (EnDat 2.2 only)
| P2 Status (03.172)
Motor pole pairs for the currently active motor | Motor pole pairs for the currently active motor

Encoder Simulation Output

Freeze System

The drive has two freeze functions that can capture the position from either the P1 or P2 position interface in the drive when a freeze trigger event occurs. A common freeze logic system is also provided, so that the freeze trigger events can be combined either to trigger the freeze system in the drive or to generate a freeze trigger for option modules. The freeze system is shown in the diagram below.

Position feedback interface thermistor input

Parameter | 03.001 Frequency Slaving Demand
--- | ---
Short description | Shows the fundamental drive output frequency when frequency slaving is enabled
Mode | Open‑Loop
Minimum | -1000.0 | Maximum | 1000.0
Default |  | Units | Hz
Type | 16 Bit Volatile | Update Rate | 4ms write
Display Format | Standard | Decimal Places | 1
Coding | RO, FI, ND, NC, PT

Frequency Slaving Demand (03.001) shows the fundamental drive output frequency when frequency slaving is enabled (Enable Frequency Slaving (03.013) = 1), otherwise it is always 0.0.

Frequency slaving mode is used to lock the fundamental frequency produced by the drive with an external frequency applied to the P1 position feedback input. Frequency slaving can be used to keep the shafts of two synchronous machines in lock by feeding the frequency slaving output from the master drive into the position feedback input of the slave drive. Alternatively the two machines could be operated so that the shafts rotate with an exact ratio, i.e. as though the shafts were connected by gears (see Slaving Ratio Numerator (03.014) and Slaving Ratio Denominator (03.015)). The source for frequency slaving mode may be quadrature AB signals or FD (frequency and direction) signals. The P1 position feedback interface must be set up to match the source signal type. The P1 position feedback interface does not need to be set up for the number of lines per revolution for the device as the pulses are taken directly from the interface and only scaled with the slaving ratio. If a 1024 line AB device is used (which corresponds to the default set up for the encoder simualtion output) then one revolution of the device will correspond to one revolution of the output voltage vector. The drive does not count pulses whilst it is disabled (Frequency Slaving Demand (03.001) shows 0.0), but it does maintain lock once enabled even if the direction of rotation changes. In frequency slaving mode the drive current limits are not active, however, the current magnitude limit is active and will try and limit the drive current by modifying the output voltage. If synchronous machines are used and the current required exceeds the drive magnitude limit the slave machine will pole slip.

Parameter | 03.005 Zero Speed Threshold
--- | ---
Short description | Set to the required zero speed threshold
Mode | Open‑Loop
Minimum | 0.0 | Maximum | 20.0
Default | 1.0 | Units | Hz
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 1
Coding | RW, BU

If the Post Ramp Reference (02.001) is at or below the level defined by this parameter in either direction Zero Speed (10.003) = 1, otherwise Zero Speed (10.003) = 0.

Parameter | 03.006 At Speed Lower Limit
--- | ---
Short description | Set to the required minimum at speed threshold
Mode | Open‑Loop
Minimum | 0.0 | Maximum | 599.0
Default | 1.0 | Units | Hz
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 1
Coding | RW

At Speed (10.006) is set if the Post Ramp Reference (02.001) is on the boundaries or within the at speed window. Above Set Speed (10.007) and Below Set Speed (10.005) are set if the reference is above or below the window respectively.

If Absolute At Speed Select (03.009) = 0 reference window mode is used.
The "at speed" condition is true if,

> (|Pre-ramp Reference (01.003)| - At Speed Lower Limit (03.006)) ≤ |Post Ramp Reference (02.001)| ≤ (|Pre-ramp Reference (01.003)| + At Speed Upper Limit (03.007))

(If the lower limit is less than zero then zero is used as the lower limit.)

If Absolute At Speed Select (03.009) = 1 absolute window mode is used.
The "at speed" condition is true if,

> At Speed Lower Limit (03.006) ≤ |Post Ramp Reference (02.001)| ≤ At Speed Upper Limit (03.007)

Parameter | 03.007 At Speed Upper Limit
--- | ---
Short description | Set to the required maximum at speed threshold
Mode | Open‑Loop
Minimum | 0.0 | Maximum | 599.0
Default | 1.0 | Units | Hz
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 1
Coding | RW

See At Speed Lower Limit (03.006).

Parameter | 03.008 Over Speed Threshold
--- | ---
Short description | Set to the required over speed threshold
Mode | Open‑Loop
Minimum | 0.0 | Maximum | 599.0
Default | 0.0 | Units | Hz
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 1
Coding | RW

If Over Speed Threshold (03.008) is set to a non-zero value it defines the over speed threshold. If the Post Ramp Reference (02.001) exceeds this threshold in either direction an Over Speed trip is produced. If Over Speed Threshold (03.008) is set to 0.0 the threshold is based on the variable minimum/maximum for the references and is equal to 1.2 x VM_SPEED_FREQ_REF[MAX].

Parameter | 03.009 Absolute At Speed Select
--- | ---
Short description | Indicates when the motor is running at speed
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See At Speed Lower Limit (03.006).

Parameter | 03.013 Enable Frequency Slaving
--- | ---
Short description | Set to 1 to enable frequency slaving
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | 4ms read
Display Format | Standard | Decimal Places | 0
Coding | RW

Enable Frequency Slaving (03.013) can be used to enable or disable frequency slaving even when the drive is enabled. The change from slaving to normal operation will result in the frequency ramping from the slaving frequency to the demanded frequency using whichever ramp rate that is applicable to normal operation. The change from normal operation to slaving will result in an instantaneous change to the slaving frequency. Therefore the slaving frequency should be similar to the demanded frequency before the change is made.

Parameter | 03.014 Slaving Ratio Numerator
--- | ---
Short description | Defines the numerator of the slaving ratio
Mode | Open‑Loop
Minimum | 0.000 | Maximum | 1.000
Default | 1.000 | Units |
Type | 16 Bit User Save | Update Rate | 4ms read
Display Format | Standard | Decimal Places | 3
Coding | RW

The slave frequency input can be scaled before it defines the Frequency Slaving Demand (03.001) using Slaving Ratio Numerator (03.014) and Slaving Ratio Denominator (03.015). The numerator and denominator can be adjusted whilst the drive is running without causing jumps in angle. However, if the change in ratio causes a large change in frequency, the transient current could activate the current magnitude limit or trip the drive.

Parameter | 03.015 Slaving Ratio Denominator
--- | ---
Short description | Defines the denominator of the slaving ratio
Mode | Open‑Loop
Minimum | 0.001 | Maximum | 1.000
Default | 1.000 | Units |
Type | 16 Bit User Save | Update Rate | 4ms read
Display Format | Standard | Decimal Places | 3
Coding | RW

See Slaving Ratio Numerator (03.014).

Parameter | 03.016 Reference Frame Angle
--- | ---
Short description | Displays the reference frame angle as a value from 0 to 65535 corresponding to one period of the drive output frequency
Mode | Open‑Loop
Minimum | 0 | Maximum | 65535
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | 250µs write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

The frequency slaving output is generated using the encoder simulation system from the reference frame that defines the drive output voltage angle. Reference Frame Angle (03.016) gives the reference frame angle as a value from 0 to 65535 corresponding to one period of the drive output frequency and should be used as the source for the encoder simulation system (i.e. Encoder Simulation Source (03.085) = 3.016) to provide a frequency slaving output. The encoder simulation output system set-up parameters can be used to set up the ratio between the reference frame frequency and the encoder simulation frequency and the format of the output signals. With the default values an AB type output is produced that gives a frequency that is 1024 times the drive output frequency.

Parameter | 03.027 P1 Speed Feedback
--- | ---
Short description | Displays the speed feedback from device P1
Mode | Open‑Loop
Minimum | −VM_SPEED | Maximum | VM_SPEED
Default |  | Units |
Type | 32 Bit Volatile | Update Rate | 4ms write
Display Format | Standard | Decimal Places | 1
Coding | RO, FI, VM, ND, NC, PT

Provided the set-up parameters for the position feedback device connected to the drive P1 position interface are correct P1 Speed Feedback (03.027) shows the speed derived from the feedback. The speed is given in mm/s if P1 Linear Feedback Select (03.051) = 1 and Linear Speed Select (01.055) = 1, otherwise it is given in rpm. The value shown is measured over a 16ms sliding window period, and so the ripple in this value is as defined for Speed Feedback (03.002).

Parameter | 03.028 P1 Revolution/Pole Pitch Counter
--- | ---
Short description | Displays the revolution/pole pitch counter from device P1
Mode | Open‑Loop
Minimum | 0 | Maximum | 65535
Default |  | Units |
Type | 16 Bit Power Down Save | Update Rate | 4ms write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

P1 Revolution/Pole Pitch Counter (03.028), P1 Position (03.029) and P1 Fine Position (03.030) combined give the encoder position with a resolution of 1/232 of a revolution/pole pitch as a 48 bit number. If a rotary position feedback device is being used (P1 Linear Feedback Select (03.051) = 0) then these quantities relate directly to the rotary position of the feedback device. If a linear feedback device is used then one revolution or pole pitch relates to the distance given by P1 Pole Pitch (03.055).

Provided the position feedback interface set-up parameters are correct, the position is always converted to units of 1/232 of a revolution/pole pitch, but some parts of the value may not be relevant depending on the resolution of the feedback device. For example a 1024 line digital encoder produces 4096 counts per revolution, and so the position is represented by the bits in the shaded area only.

When the position feedback moves by more than one revolution or pole pitch the P1 Revolution/Pole Pitch Counter (03.028) increments or decrements in the form of a sixteen bit roll-over counter. If an absolute position feedback device (except AB Servo, FD Servo, FR Servo, SC Servo) is used the position is initialised at power-up and each time the encoder is subsequently initialised with the absolute position including the revolution count if a multi-turn absolute rotary encoder is used, or the pole pitch count if an absolute linear encoder is used. To avoid showing turns values that are outside the range of the encoder any bits beyond the turns information are normally masked. For example, if the encoder provides 12 bits of turns information, then the most significant 4 bits of the revolutions are always zero. If a single turn encoder is used all the bits of the revolutions are zero. To remove this masking P1 Absolute Turns Recovery Enable (03.073) should be set to one. In addition to removing the mask, the extended turns value is retained on power-down and will be recovered on power-up. See P1 Absolute Turns Recovery Enable (03.073) for more details.

The position interface parameter descriptions cover rotary and linear applications, but the revolutions or pole pitches are always referred to as turns.

Parameter | 03.029 P1 Position
--- | ---
Short description | Displays the position feedback from device P1
Mode | Open‑Loop
Minimum | 0 | Maximum | 65535
Default |  | Units |
Type | 16 Bit Power Down Save | Update Rate | 4ms write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

See P1 Revolution/Pole Pitch Counter (03.028).

Parameter | 03.030 P1 Fine Position
--- | ---
Short description | Displays the fine position feedback from device P1
Mode | Open‑Loop
Minimum | 0 | Maximum | 65535
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | 4ms write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

See P1 Revolution/Pole Pitch Counter (03.028).

Parameter | 03.031 P1 Marker Mode
--- | ---
Short description | Defines the marker mode for device P1
Mode | Open‑Loop
Minimum | 0 (Display: 0000) | Maximum | 15 (Display: 1111)
Default | 4 (Display: 0100) | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Binary | Decimal Places | 0
Coding | RW

P1 Device Type (03.038): AB, FD, FR, AB Servo, FD Servo, FR Servo
Each position feedback device produces incremental signals which are counted in hardware. If P1 Marker Mode (03.031) = 0 the following occurs when a marker event is produced by the Z1 input:

1. P1 Position (03.029) and P1 Fine Position (03.030) are reset to zero.
2. The bits in P1 Normalised Position (03.058) related to P1 Position (03.029) and P1 Fine Position (03.030) are reset to zero
3. P1 Marker Flag (03.032) is set to one.

The marker is a hardware function, and so the position appears as though it is reset at the marker event time even if this is between control system sample points. It should be noted that the marker event occurs on the rising edge of the marker pulse if the position change over the last sample was positive or on the falling edge if the position change over the last sample was negative. This ensures that the marker event occurs at the same physical location for either direction of rotation.

The action taken when a marker event occurs can be modified by setting the bits of P1 Marker Mode (03.031) as described in the table below.

Bit | Effect of setting bit to one
0 | No action is taken unless the marker flag is zero before the marker event occurs
1 | P1 Revolution/Pole Pitch Counter (03.028) and the whole of P1 Normalised Position (03.058) are also set to zero on a marker event
2 | P1 Revolution/Pole Pitch Counter (03.028), P1 Position (03.029), P1 Fine Position (03.030) and the related part of P1 Normalised Position (03.058) are not reset. (This overrides bit 1.) P1 Normalised Position (03.058) is transferred to P1 Normalised Marker Position (03.059) and P1 Marker Flag (03.032) is set to one.
3 | If this bit is 0 the state of the marker is only undefined when the differential input is in the range from -200mV to 200mV. The marker pulse is only guaranteed to be recognised if it is at least 500ns wide. This setting is used for most encoders with standard level marker pulses. If this bit is set to 1 the undefined state region is reduced to the range from -30mV to 30mV. The marker pulse is only guaranteed to be recognised if it is at least 10us wide. The smaller undefined region is required for position feedback devices that produce a small marker pulse, such as the Heidenhain ERN1387 encoder. Note that the reduced undefined region is only provided for position feedback interface P1 and that this bit in P2 Marker Mode (03.131) has not effect.

The marker input can be used for a standard type marker function or alternatively it can be used as an additional freeze input for the P1 position feedback interface.

P1 Device Type (03.038): SC, SC Servo, SC SC
The marker function operates in the same way as for the digital incremental encoders. The resolution of the marker actions is only as accurate as the zero crossings of the sine waves. The marker is used with an SC SC type device to trim the absolute position derived from the single sine wave per turn channels once after initialisation. Until this is done (i.e. the marker has been active once after initialisation) marker events will not be registered.

P1 Device Type (03.038): Any other device type
The marker function cannot be used and P1 Marker Mode (03.031) has no effect.

Parameter | 03.032 P1 Marker Flag
--- | ---
Short description | Indicates when a marker event occurs
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit Volatile | Update Rate | 250µs write
Display Format | Standard | Decimal Places | 0
Coding | RW, NC

P1 Marker Flag (03.032) is set to one when a marker event occurs. The flag must be cleared by the user.

Parameter | 03.033 P1 Rotary Turns Bits
--- | ---
Short description | Defines the number of rotary turns bits for device P1
Mode | Open‑Loop
Minimum | 0 | Maximum | 16
Default | 16 | Units |
Type | 8 Bit User Save | Update Rate | Background read, auto-configuration write
Display Format | Standard | Decimal Places | 0
Coding | RW

P1 Rotary Turns Bits (03.033) normally only has any effect if the position feedback interface is being used with a rotary device (i.e. P1 Linear Feedback Select (03.051) = 0).

P1 Device Type (03.038): SC Hiperface, SC EnDat, SC SSI, EnDat, BISS, SSI, SC BiSS
P1 Rotary Turns Bits (03.033) is used to determine the number of bits within the comms messages from the position feedback device that represent turns. For a single turn encoder P1 Rotary Turns Bits (03.033) must be set to zero. The most significant bits in P1 Revolution/Pole Pitch Counter (03.028) that are not included in the turns information provided by the encoder comms are held at zero. If P1 Rotary Turns Bits (03.033) = 0 (single turn encoder) the whole of P1 Revolution/Pole Pitch Counter (03.028) is held at zero. The number of bits of position information within one revolution for a rotary device are calculated from P1 Rotary Turns Bits (03.033) and P1 Comms Bits (03.035). If the resulting value is greater than 32 it is limited to 32.

Some SSI encoders include leading zeros before the turns information and in this case the number of turns bits should include the leading zeros. Some BiSS encoders include zero padding either before or after the turns information (see P1 Additional Configuration (03.074)). P1 Rotary Turns Bits (03.033) should include the actual turns bits and the additional padding.

P1 Device Type (03.038): Option Slot 1, Option Slot 2, Option Slot 3, Option Slot 4
Whatever the setting for P1 Linear Feedback Select (03.051) the number of rotary turns bits should be set up to indicate how many turns bits there are in the position provided by an option module. See P1 Device Type (03.038) for more details.

P1 Device Type (03.038): Any other device type
It is sometimes desirable to mask off the most significant bits of P1 Revolution/Pole Pitch Counter (03.028), but this does not have to be done for the drive to function correctly. If P1 Rotary Turns Bits (03.033) = 0 the whole of P1 Revolution/Pole Pitch Counter (03.028) is held at zero. If P1 Rotary Turns Bits (03.033) has any other value it indicates the number of bits in P1 Revolution/Pole Pitch Counter (03.028) that are not held at zero. For example, if P1 Rotary Turns Bits (03.033) = 5, then P1 Revolution/Pole Pitch Counter (03.028) counts up to 31 before being reset.

The description above is for normal operation when P1 Absolute Turns Recovery Enable (03.073) = 0. If P1 Absolute Turns Recovery Enable (03.073) = 1 no masking is applied to P1 Rotary Turns Bits (03.033), and so a 16 bit value is always shown.

Parameter | 03.034 P1 Rotary Lines Per Revolution
--- | ---
Short description | Defines the number of rotary lines per revolution for device P1
Mode | Open‑Loop
Minimum | 1 | Maximum | 100000
Default | 1024 | Units |
Type | 32 Bit User Save | Update Rate | Background read, auto-configuration write
Display Format | Standard | Decimal Places | 0
Coding | RW

P1 Rotary Lines Per Revolution (03.034) only has any effect if the position feedback interface is being used with a rotary device (i.e. P1 Linear Feedback Select (03.051) = 0).

P1 Device Type (03.038): AB, AB Servo
P1 Rotary Lines Per Revolution (03.034) should be set to the number of lines per revolution for the encoder connected to the P1 position feedback interface.

P1 Device Type (03.038): FD, FR, FD Servo, FR Servo
P1 Rotary Lines Per Revolution (03.034) should be set to the number of lines per revolution for the encoder connected to the P1 position feedback interface divided by 2.

P1 Device Type (03.038): SC, SC Servo, SC Hiperface, SC EnDat, SC SSI, SC SC, SC BiSS
P1 Rotary Lines Per Revolution (03.034) should be set to the number of sine waves per revolution for the encoder connected to the P1 position feedback interface.

P1 Device Type (03.038): Any other device type
P1 Rotary Lines Per Revolution (03.034) has no effect.

Parameter | 03.035 P1 Comms Bits
--- | ---
Short description | Defines the total number of bits of position information in the comms message from the encoder for device P1
Mode | Open‑Loop
Minimum | 0 | Maximum | 48
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read, auto-configuration write
Display Format | Standard | Decimal Places | 0
Coding | RW

P1 Device Type (03.038): SC Hiperface, EnDat, SC EnDat
Total number of bits of position information in the comms message from the encoder.

P1 Device Type (03.038): SSI, SC.SSI
Total number of bits of position information in the comms message from the encoder including any leading or trailing zeros and the power supply alarm bit if present.

P1 Device Type (03.038): BiSS, SC BiSS
Total number of bits of position information in the comms message from the encoder excluding the warning and error bits. It is always assumed there is one warning bit and one error bit. The length of the position information includes any zero padding that is included by the encoder.

P1 Device Type (03.038): Any other device type
P1 Comms Bits (03.035) has no effect.

Parameter | 03.036 P1 Supply Voltage
--- | ---
Short description | Defines the supply voltage output for device P1
Mode | Open‑Loop
Minimum | 0 | Maximum | 2
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | 5V
1 | 8V
2 | 15V

P1 Supply Voltage (03.036) sets the level for the supply voltage output. To ensure that the maximum voltage for the position feedback device is not accidentally exceeded, the device should be disconnected from the drive when the level is being adjusted.

Parameter | 03.037 P1 Comms Baud Rate
--- | ---
Short description | Defines the baud rate used for encoder communications
Mode | Open‑Loop
Minimum | 0 | Maximum | 8
Default | 2 | Units | Baud
Type | 8 Bit User Save | Update Rate | Background read, Auto-configuration write
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | 100k
1 | 200k
2 | 300k
3 | 400k
4 | 500k
5 | 1M
6 | 1.5M
7 | 2M
8 | 4M

P1 Comms Baud Rate (03.037) defines the baud rate used for encoder communications. Restrictions are applied to the baud rate for different feedback devices, and so the baud rate may be different to the parameter value.

P1 Device Type (03.038): SC.Hiperface
A fixed baud rate of 9600 baud is always used with this type of encoder so P1 Comms Baud Rate (03.037) has no effect.

P1 Device Type (03.038): SC.SSI, SC EnDat, SC BiSS
Any baud rate that is within the range specified for the encoder may be used. The data from the encoder is not used for time critical functions, and so it is recommended that the default value of 300K baud is used unless this needs to be reduced because of a limitation imposed by the encoder.

P1 Device Type (03.038): EnDat, BiSS, SSI
Any baud rate that is within the range specified for the encoder may be used. The line delay is measured during initialisation, and used to compensate this delay during communications with the encoder. Therefore there is no timing based restriction on the length of the cable between the position feedback interface and the encoder. However, care should be taken to ensure that the wiring arrangement and the type of cable used are suitable for the selected baud rate and the distance between the position interface and the encoder. See P1 Low Speed Update Rate Active (03.063) for more details on timing restrictions related to the drive sample times.

P1 Device Type (03.038): Any other device
P1 Comms Baud Rate (03.037) has no effect.

Parameter | 03.038 P1 Device Type
--- | ---
Short description | Defines the device type connected to the drive P1 position feedback interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 20
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | AB
1 | FD
2 | FR
3 | AB Servo
4 | FD Servo
5 | FR Servo
6 | SC
7 | SC Hiperface
8 | EnDat
9 | SC EnDat
10 | SSI
11 | SC SSI
12 | SC Servo
13 | BiSS
14 | Resolver
15 | SC SC
16 | Commutation Only
17 | SC BiSS
18 | Option Slot 1
19 | Option Slot 2
20 | Option Slot 3

P1 Device Type (03.038) should be set up to match the device connected to the drive P1 position feedback interface. The table below gives the position feedback types supported by the P1 position feedback interface.

P1 Device Type (03.038) | Signals | Position feedback type | Communications
0: AB | Quadrature | Incremental | None
1: FD | Frequency and direction | Incremental | None
2: FR | Forward and reverse | Incremental | None
3: AB Servo | Quadrature and commutation | Absolute commutation signals with incremental | None
4: FD Servo | Frequency and direction, and commutation | Absolute commutation signals with incremental | None
5: FR Servo | Forward and reverse, and commutation | Absolute commutation signals with incremental | None
6: SC | SINCOS | Incremental SINCOS | None
7: SC Hiperface | SINCOS and Hiperface comms | Absolute comms with incremental SINCOS | Hiperface
8: EnDat | EnDat comms | Absolute comms | EnDat 2.1 EnDat 2.2
9: SC EnDat | SINCOS and EnDat comms | Absolute comms with incremental SINCOS | EnDat 2.1
10: SSI | SSI comms | Absolute comms | SSI
11: SC SSI | SINCOS and SSI comms | Absolute comms with incremental SINCOS | SSI
12: SC Servo | SINCOS and commutation | Absolute commutation signals with incremental | None
13: BiSS | BiSS comms | Absolute comms | BiSS
14: Resolver | Resolver | Resolver | None
15: SC SC | SINCOS and single sine and cosine signals per revolution | SINCOS with absolute position from single sine and cosine signals | None
16: Commutation Only | Commutation only | Absolute commutation signals only | None
17: SC BiSS | BiSS comms | Absolute comms with incremental SINCOS | BiSS
18: Option Slot 1 | None | Provided by option module | None
19: Option Slot 2 | None | Provided by option module | None
20: Option Slot 3 | None | Provided by option module | None
21 Option Slot 4 | None | Provided by option module | None

Position feedback type:

Incremental
Position devices that provide incremental feedback do not give absolute position feedback. The position is zero at power-up and accumulates the change of position from that point on. These devices are suitable for motor control in RFC-A mode. They can also be used for RFC-S mode, but some form of phasing auto-tune is required each time the position feedback is initialised.

Absolute commutation signals with incremental
Position devices with commutations signals are intended to provide absolute position feedback for motor control in RFC-S mode. If one of these devices is used for RFC-A mode the commutation signals are ignored. The position information given in P1 Revolution/Pole Pitch Counter (03.028), P1 Position (03.029) and P1 Fine Position (03.030) appears as though the position feedback device is an incremental type in that it is initialised to zero at power-up and then accumulates the change of position from that point on. The commutation signals are used directly by the motor control algorithms in RFC-S mode to determine the motor position after position feedback initialisation. There must be one period of the commutation signals for each pole pair for a rotary motor (i.e. 3 commutation signal periods per revolution for a 6 pole motor), or one period of the commutation signals must be equal to the motor pole pitch for a linear motor. It should be noted that for a movement of up to 1/3 of the commutation signal period after position feedback initialisation the maximum motor torque is limited to 0.866 of the maximum possible torque.

Absolute commutation signals only
Position devices with commutations signals are intended to provide absolute position feedback for motor control in RFC-S mode but can also be used to provide position feedback for motor control in RFC-A mode. The position is derived from the commutation signals alone. A phase locked loop is used to smooth the feedback, but this introduces a delay and there is significant ripple in the position and speed feedback at low speeds. If this method is used for motor control then low speed loop gains should be used and P1 Feedback Filter (03.042) should be used to filter the feedback.

Incremental SINCOS
An incremental SINCOS encoder can be used in the same way as an AB incremental encoder, except that the position resolution is increased with interpolation. These devices are suitable for motor control in RFC-A mode. They can also be used for RFC-S mode, but some form of phasing auto-tune is required each time the position feedback is initialised. The increase in resolution due to interpolation depends on the magnitude and frequency of the sine wave signals at the position feedback interface inputs on the drive. The sine wave inputs take balanced signals each with a nominal 1V peak to peak level. (This means that the difference measured between the two signals for one sine wave input would be 2V peak to peak or 1V peak.) If interpolation is not used the position feedback would have a resolution related to the number of sine waves per revolution (i.e. 512 sine waves per revolution would give position feedback resolution equivalent to a 512 line incremental encoder, which gives 2048 discernible positions per revolution). With the nominal signal level and an input frequency below 5kHz the interpolation using sine waves instead of digital incremental signals increases the resolution by a factor of 1800. For a 512 sine wave encoder this would give a resolution of 512 x 4 x 1800 = 3686400 discernible positions per revolution. This is equivalent to a digital incremental encoder with 921600 lines per revolution.The increased resolution due to interpolation is directly proportional to the sine wave signal voltage levels, and also reduces with sine wave signal frequency. The resolution is given by

Resolution = P1 Rotary Lines Per Revolution (03.034) x 4 x 1800 x Vpeak to peak of the sine wave signals x Frequency Factor

where the frequency factor is given below.

1kHz | 5kHz | 50kHz | 100kHz | 200kHz | 500kHz
1.00 | 1.00 | 0.86 | 0.66 | 0.39 | 0.14

Increasing the sine wave signal level above 1V peak to peak will increase the resolution, but the level should not be increased above 1.5V or else the input will saturate and the sine waves will be distorted.

Absolute comms with incremental SINCOS
The absolute position is obtained after position feedback initialisation via the comms interface and then after that point by tracking the incremental change from the sine wave signals. Interpolation is used to increase the position resolution. The comms interface can be used to check the position derived from the sine waves. It can also be used for bi-direction transfer of data between the drive and encoder (except SSI comms). These devices can be used for motor control in RFC-A or RFC-S modes.

Absolute comms
The absolute position is obtained at all times via the encoder comms. The comms interface can also be used for bi-directional transfer of data between the drive and the encoder (except SSI mode). These devices can be used for motor control in RFC-A or RFC-S modes.

Resolver
A resolver can be used to provide absolute position feedback within the range covered by one electrical revolution of the resolver (i.e. 360° mechanical for a 2 pole device, 180° mechanical for a 4 pole device, etc.). An angle of 0 degrees corresponds to the position where the cosine input is at its maximum and in phase with the excitation and the sine input zero. A resolver can be used for motor control in RFC-A mode or RFC-S mode. In RFC-S mode a 2 pole resolver can be used with a motor with any number of motor poles, but with any other number of poles there must be an integer number of motor poles for each resolver pole. In RFC-A mode this restriction does not apply. Standard or high speed sampling can be selected with P1 Resolver Excitation (03.066). If standard sampling is selected and the position feedback used for motor control the maximum operating speed is limited before the control peroformance starts to deteriorate. See P1 Resolver Excitation (03.066) for more details.

SINCOS with absolute position from sine and cosine signals
This type of device, which is not recommended for new applications, is intended to provide absolute position feedback for motor control in RFC-S mode. If one of these devices is used for RFC-A mode the additional sine wave signals and the Z1 marker signal do not affect the motor control position feedback. The position information given in P1 Position (03.029) and P1 Fine Position (03.030) is initialised to the position within one turn and P1 Revolution/Pole Pitch Counter (03.028) is set to zero when the device is initialised based on the once per turn sine and cosine signals. This gives a moderately accurate absolute position. When a marker event occurs it is used to give a more accurate absolute position. Care should be taken to ensure that the position feedback device is connected correctly. For example a Heidenhain ERN1387 device should be connected as follows: 1/2=A+/A-(Cosine), 3/4=B+/B-(Sine), 5/6=R+/R-(Marker), 7/8=C+/C-(Single turn cosine), 9/10=D+/D-(Single turn sine). It is assumed that the marker occurs at the positive zero crossing of the single turn cosine signal when operating in the forwards direction (i.e. compatible with the ERN1387). To ensure the drive can correctly detect the reference marker pulse with a Heidenhain ERN1387 encoder it is recommended that bit 3 of P1 Marker Mode (03.031) is set to 1.

Provided by Option Module
Position feedback information can be provided via the P1 interface from an option module. This is intended to be used by option modules that are not position feedback category modules. If this type of device is selected, and the module in the selected slot supports this feature, the position provided by the P1 interface will be written by the module and the interface will become initialised. If the option does not support this feature then the position will remain at zero and the interface will not become initialised. It should be noted that the system allows 1.3s after power-up, or feedback interface re-initialisation, for the option module to indicate that it is providing feedback before a Encoder 4 trip will be initiated. If the option module takes longer than this to indicate that position feedback is available the power up delay should be extended with P1 Additional Power-up Delay (03.049).

The option module will provide the postion as a 32 bit value separated into turns and position within a turn as shown below.

Turns | Position

The number of turns bits should be set up in P1 Rotary Turns Bits (03.033) and the position value should be left justified. For example, if the information being provided contains 8 turns bits and 16 position bits then P1 Rotary Turns Bits (03.033) should be set to 8 and the information should be written as shown below.

8 turns bits | 16 position bits | 8 zeros

For a linear device P1 Rotary Turns Bits (03.033) should be used in the same way to partition the data from the module where one turn corresponds to one pole of the motor.

To avoid discontinuities when the whole position rolls over the maximum number of turns boundary, the drive calculates the change of position between the values provided by the option module at each sample and then accumulates the result. It is important that the change of position provide by the option module between samples is less than half the range of the position value. For example, if 16 position bits are being used the change must be less than 32767. This only applies when the position feedback interface is in the initialised state. If it is not initialised then larger changes can be applied.

Communications:

Hiperface
Hiperface is an asynchronous bi-direction communications protocol that is only used with incremental sine waves. Therefore it can be used to check the position derived from the sine waves or for bi-direction transfer of data between the drive and encoder. A checksum is provided for error checking.

EnDat 2.1
EnDat 2.1 is a synchronous bi-direction communications protocol that is intended to be used with incremental sine waves. Therefore it can be used to check the position derived from the sine waves or for bi-direction transfer of data between the drive and encoder. It can be used as an absolute comms only type position feedback interface, but the resolution of the position feedback using this method may be limited. If it is used in this way it is not possible to use the position feedback via comms at the same time as communicating with the encoder for data transfer. A CRC is provided for error checking.

EnDat 2.2 and BiSS C Mode
EnDat 2.2 and BiSS are synchronous bi-direction communications protocols that are intended to be used alone. It is possible to obtain position feedback at the same time as communicating with the encoder for data transfer. A CRC is provided for error checking.

SSI
SSI is a uni-directional communications protocol that is intended to be used alone. It is only possible to obtain the position information from the encoder and it is not possible to transfer data between the drive and the encoder. No error checking is provided by the SSI protocol, and so encoders based on this interface are not recommended for new applications.

Parameter | 03.039 P1 Termination Select
--- | ---
Short description | Used to enable or disable the terminations on the position feedback interface inputs
Mode | Open‑Loop
Minimum | 0 | Maximum | 2
Default | 1 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

P1 Termination Select (03.039) is used to enable or disable the terminations on the position feedback interface inputs. The function of P1 Termination Select (03.039) depends on the position feedback device type selected in P1 Device Type (03.038) as shown below.

Terminals 5/6 have selectable pull-apart resistors which follow the same state as the termination resistors for terminals 5/6, unless described differently below.

P1 Device Type (03.038): AB, FD, FR, AB Servo, FD Servo, FR Servo

Terminal | Input | 03.039 = 0 | 03.039 = 1 | 03.039 = 2
1/2 & 3/4 | A1 & B1 | Disabled | Enabled | Enabled
5/6 | Z1 | Disabled | Disabled | Enabled

U1, V1 & W1 terminations (terminals 7/8, 9/10 & 11/12) are always enabled for AB Servo, FD Servo and FR Servo encoders.

P1 Device Type (03.038): SC, SC Servo, SC SC

Terminal | Input | 03.039 = 0 | 03.039 = 1 | 03.039 = 2
1/2 & 3/4 | Cos1 & Sin1 | Disabled | Enabled | Enabled
5/6 | Z1 | Disabled | Disabled | Enabled

U1, V1 & W1 (terminals 7/8, 9/10 & 11/12) terminations are always enabled for SC Servo encoders. SCs1 and SSn1 (terminals 7/8 & 9/10) terminations are always enabled for SC SC encoders.

P1 Device Type (03.038): SC Hiperface, SC EnDat, SC SSI, SC BiSS

Terminal | Input | 03.039 = 0 | 03.039 = 1 | 03.039 = 2
1/2 & 3/4 | Cos1 & Sin1 | Disabled | Enabled | Enabled
5/6 | D1 | Enabled | Enabled | Enabled

For SC EnDat and SC SSI encoder the pull-apart resistors on the D1 input/output (terminals 5/6) are always disabled, and for SC Hiperface encoders the pull-apart resistors on the D1 input/output (terminals 5/6) are always enabled.

P1 Device Type (03.038): EnDat, BiSS, SSI

Terminal | Input | 03.039 = 0 | 03.039 = 1 | 03.039 = 2
1/2 & 3/4 | D1/CLK1 | Enabled | Enabled | Enabled
5/6 | Z1 | Disabled | Disabled | Enabled

If the P2 Device type (03.138) is set to EnDat, BiSS or SSI and the encoder simulation output is enabled, then the Z1 input becomes the data (D2) input for the P2 position interface and termination resistors are always enabled and pull-apart resistors are always disabled.

P1 Device Type (03.038): Resolver
P1 Termination Select (03.039) has no effect as terminations are always disabled.

P1 Device Type (03.038): Commutation Only
P1 Termination Select (03.039) has no effect as terminations are always enabled.

Parameter | 03.040 P1 Error Detection Level
--- | ---
Short description | Used to enable or disable position feedback trip functions
Mode | Open‑Loop
Minimum | 0 (Display: 00000000) | Maximum | 255 (Display: 11111111)
Default | 0 (Display: 00000000) | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Binary | Decimal Places | 0
Coding | RW, BU

This parameter can be used to enable or disable position feedback trip functions as follows:

Bit | Function | Trip(s) | Comments
0 | Enable wire break detection. | Encoder 2 | Bits 5 and 6 have no effect if this bit is set to zero.
1 | Enable phase error detection. | Encoder 3 |
2 | Enable SSI power supply alarm bit monitor. | Encoder 6 |
3 | Disable indicated trips. | Encoder 1 to Encoder 6 | Trips related to bits 0, 1, 2, 5 and 6 do not ocur if this bit is set to one. See note below about the position feedback device becoming uninitialised.
4 | Disable indicated trip. | Encoder 7. |
5 | Enable wire break detection for sine wave commutation signals for SC SC type encoders. | Encoder 2 |
6 | Enable wire break detection for the marker with SC SC type encoders with Heidenhain ERN1387 type marker signals. | Encoder 2 |
7 | Enable more sensitive resolver wire break detection. | Encoder 2 | The standard wire break detection is only likely to detect a break in the excitation signal, or both the sine and cosine signals together. The more sensitive system will detect a break in any signal provided the motor is rotating. If the motor is stationary, there are positions where wire break will not be detected. The standard system uses 10% of the expected 1Vrms feedback signals as the detection threshold, but the more sensitive system uses 80%. If the resolver ratio is significantly less than 3:1 with 3V excitation, or 2:1 with 2V excitation, then the more sensitive detection system should not be used.

Bits 3 and 4 do not prevent the device from becoming un-initialised. The trip is suppressed, but the device is still un-initialised and this is indicated by the appropriate bit for the position feedback interface in Position Feedback Initialized (03.076).

Encoder trips
The following table shows trips that can be initiated that are related to the position feedback interface P1. The sub-trip number is 1 for the drive P1 position feedback interface.

Drive trip | Encoders | Reason for error
Encoder 1 | All | Power supply short circuit
Encoder 2 | AB, FD, FR, AB Servo, FD Servo, FR Servo | Hardware wire-break detect on A1, B1 and Z1 inputs 1. (Note that there is no wire break detection on the U1, V1 and W1 commutation inputs.)
SC, SC Servo, SC Hiperface, SC EnDat, SC SSI, Resolver, SC SC, SC BiSS | Software wire break detection on sine wave signals. Marker and single turn sine wave commutation signals for SC SC device5. (Note that there is no wire break detection on the U1, V1 and W1 commutation inputs.)
Encoder 3 | AB Servo, FD Servo, FR Servo, SC Servo | Phase error 2
SC Hiperface, SC EnDat, SC SSI, SC BiSS | Sine/cosine phase error 3
Encoder 4 | SC Hiperface, SC EnDat, EnDat, BISS, SC BiSS Option Slot 1, Option Slot 2, Option Slot 3, Option Slot 4 | Comms timeout The option module in the selected option slot has not indicated that it is providing position feedback.
Encoder 5 | SC Hiperface, SC EnDat, EnDat, BISS, SC BiSS | Checksum/CRC error
SC SSI, SSI | Not ready at start of position transfer (i.e. data input not one)
Encoder 6 | SC Hiperface, SC EnDat, EnDat, BiSS, SC BiSS | The encoder has indicated an error
SSI, SC SSI | Power supply alarm bit active
Encoder 7 | All | A set-up parameter for the device or the number of pole pairs for the currently selected motor have been changed.
Encoder 8 | EnDat, SSI, BiSS | P1 Device Type (03.038), P1 Comms Bits (03.035), P1 Comms Baud Rate (03.037), P1 Calculation Time (03.060), P1 Recovery Time (03.061), P1 Line Delay Time (03.062) and P1 User Comms Enable (03.067) are used to determine the time taken for the communications exchange with the encoder. If this time exceeds 250μs an Encoder 8 trip is initiated.
Encoder 9 | All | Speed feedback selected from an option slot that does not have a position feedback category option module fitted
Phasing Error | All | Incorrect encoder phasing 4
Encoder 12 | SC Hiperface, BiSS | The encoder could not be identified during auto-configuration
Encoder 13 | SC Hiperface, SC EnDat, EnDat, BiSS, SC BiSS | Data read from the position feedback device during auto-configuration is out of range
Encoder 14 | BiSS, SC BiSS | The turns or position padding values in parameter P1 Additional Configuration (03.074) are out of range.

1. If the terminations are not enabled on the A1, B1 or Z1 inputs the wire break system will not operate. (Note that as default the Z1 input terminations are disabled to disable wire break detection on this input.)
2. Phase error detection for AB Servo, FD Servo, FR Servo or SC Servo encoders monitors the relationship between the position from the incremental signals and the commutation signals to ensure that the incremental pulses have been counted correctly. The error is detected if the incremental position moves outside the position range defined by the UVW commutation signals by 10o. The trip is initiated if the error is detected for 10 consecutive samples. This system should not be used unless one encoder line (AB Servo), or two lines (FD Servo, FR Servo), are less than 10° electrical or else spurious Encoder 3 trips will occur.
3. Phase error detection for SINCOS encoders with comms monitors the relationship between the position derived from the sine waves with the position derived via comms. The encoder is interrogated via comms and the comparison is made once per second. If the error is greater than 10° electrical for 10 consecutive samples the trip is initiated. This system should not be used unless one sine wave is less than 10° electrical or else spurious Encoder 3 trips will occur.
4. Incorrect encoder phasing is detected if the motor reaches half of the speed defined by VM_SPEED_FREQ_REF[MAX] and the phasing error is large enough for the motor to accelerate uncontrollably.
5. Detection of wire break on the sine wave commutation signals or marker of an SC SC device may require the encoder to rotate by several mechancial turns before the fault is detected, i.e. up to 2 turns for the sine wave commutation signals and up to 3 turns for the marker).

Wire-break detection
It may be important to detect a break in the connections between the drive and the position feedback device. This feature is provided for most position feedback devices either directly or indirectly as listed below.

Device | Detection method | Trip produced
AB, FD, FR, AB Servo, FD Servo, FR Servo | Hardware detectors on the A1, B1 and Z1 signal detect a wire break. | Encoder 2
SC, SC Servo, SC Hiperface, SC EnData, SC SSI, SC SC, SC BiSS | The magnitudes of the sine wave signals are monitored as the magnitude of a vector which is calculated as √(Sine2+Cosine2). If this is less than the value produced by two valid waveforms with a peak to peak magnitude of 0.25V (i.e. 0.25 of the nominal level of 1V peak to peak) then a trip is initiated. This always detects wire break in the sine and cosine connections if the position feedback is changing. If the position feedback is stationary this may not detect wire break until the position feedback moves, e.g. if the sine connection is broken, but the cosine is at it's maximum then wirebreak will not be detected. Additional monitoring is provided for SC SC encoders to give software wire break detection for the single turn sine wave commutation signals and the marker. If the device is a Heidenhain ERN1387 the marker is too small for hardware wire break detection, and so the additional software detection is required to detect wire break on the marker. | Encoder 2
Resolver | The magnitudes of the sine and cosine input signals are monitored in a similar way to SINCOS signals where the peak of the sine and cosine waveforms are used to calculate the vector magnitude. If the caclulated value is less than the value produced by two valid waveforms with a differential peak to peak magnitude of 0.4V then a trip is initiated. This detects wire break in the sine and cosine connections. If the position feedback is stationary this may not detect wire break until the position feedback moves, e.g. if the sine connection is broken, but the cosine is at it's maximum then wirebreak will not be detected. | Encoder 2
SC Hiperface, SC EnDat, EnDat, BiSS, SC BiSS | Wire break in the comms link is detected by a CRC or timeout error. | Encoder 4, Encoder 5
SSI, SC SSI | Wire break detection in the comms is difficult with these devices. However, if power supply alarm bit monitoring is enabled the drive will be looking for a one at the start of the message and a zero to indicate that the power supply is okay. If the clock stops or the data line is disconnected the data input to the drive may stay in one state or the other and cause a trip. | Encoder 5, Encoder 6

Position feedback power supply trips
The position feedback power supply from the drive can be switched off by the drive either because the power supply is overloaded (Encoder 1 trip) or because the internal 24V supply within the drive is overloaded (PSU 24V trip). The internal 24V supply provides power for the position feedback power supply, user 24V output, digital I/O, option modules etc. To ensure that an Encoder 1 trip is not initiated when the internal 24V is overloaded, and subsequently switched off by the drive, there is a delay of 40ms in the detection of Encoder 1 trip. It is possible for other position feedback trips, such as wire break detection (i.e. Encoder 2), to occur when the power supply is removed from the position feedback device. Therefore overloading the internal 24V supply or the position feedback supply could result in an immediate Encoder 2 trip. To ensure that the correct reason for the trip is given PSU 24V and Encoder 1 trips override an existing Encoder 2 to Encoder 6 trip. This means that both the original trip (Encoder 2 to Encoder 6) and then the new trip (PSU 24V or Encoder 1) are stored in the trip log.

Parameter | 03.041 P1 Auto-configuration Select
--- | ---
Short description | Set to 1 to enable interrogation of the encoder to determine the set up required
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 1 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Disabled
1 | Enabled

P1 Device Type (03.038): SC Hiperface, SC EnDat, EnDat, BiSS, SC BiSS
If auto-configuration has not been disabled (i.e. P1 Auto-configuration Select (03.041) is not 0) then during position feedback initialisation the encoder is interrogated to determine whether the encoder is a rotary or linear encoder and P1 Linear Feedback Select (03.051) is set up appropriately. Then the following parameters are set up based on information from the encoder:

Rotary | Linear
P1 Rotary Turns Bits (03.033) | P1 Linear Comms Pitch (03.052)
P1 Rotary Lines Per Revolution (03.034) | P1 Linear Line Pitch (03.053)
P1 Comms Bits (03.035) | P1 Comms Bits (03.035)
P1 Additional Configuration (03.074) | P1 Linear Comms And Line Pitch Units (03.054)

The following actions are also taken to set up the timing for the encoder.

Comms Protocol | Actions taken
EnDat 2.1 | P1 Calculation Time (03.060) = From the encoder P1 Recovery Time (03.061) = 30μs Line delay measured and result written to P1 Line Delay Time (03.062)
EnDat 2.2 | P1 Calculation Time (03.060) = From the encoder P1 Recovery Time (03.061) is set to 4μs (and the encoder itself is set up to use its short recovery time of 3.75μs) if the P1 Comms Baud Rate (03.037) is 1M or more. Line delay measured and result written to P1 Line Delay Time (03.062)
BiSS | P1 Absolute Turns Recovery Enable (03.073) = 5μs P1 Recovery Time (03.061) = 13μs Line delay measured and result written to P1 Line Delay Time (03.062)

Once these parameters have been set up it should be possible for the drive to operate correctly with the encoder. Auto-configuration occurs as part of the position interface initialisation if selected, and so if the auto-configuration fails (i.e. communications cannot be established) then initialisation will not be completed. If initialisation has not been completed successfully the drive cannot be enabled (see Enable Conditions (06.010)). For SC Hiperface and BiSS encoders the drive must identify the encoder model number to perform auto-configuration. If communications is established, but the drive cannot recognise the encoder model, an Encoder 12 trip is produced immediately.

If auto-configuration is disabled ((i.e. P1 Auto-configuration Select (03.041) = 0) then none of the above actions are carried out except for the line delay measurement.

P1 Device Type (03.038): All other device types
P1 Auto-configuration Select (03.041) has no effect.

Parameter | 03.042 P1 Feedback Filter
--- | ---
Short description | Defines the time period for a sliding window filter that may be applied to the feedback taken from the drive P1 position feedback interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 5
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Disabled
1 | 1ms
2 | 2ms
3 | 4ms
4 | 8ms
5 | 16ms

P1 Feedback Filter (03.042) defines the time period for a sliding window filter that may be applied to the feedback taken from the drive P1 position feedback interface. This is particularly useful in applications where the drive encoder is used to give speed feedback for the speed controller and where the load includes a high inertia, and so the speed controller gains are very high. Under these conditions, without a filter on the feedback, it is possible for the speed loop output to change constantly from one current limit to the other and lock the integral term of the speed controller. In Unidrive SP this filter was applied to the output of the sensorless speed feedback, however, a separate filter is now provided (see Sensorless Mode Filter (03.079)).

Parameter | 03.043 P1 Maximum Reference
--- | ---
Short description | Defines the maximum speed reference from device P1
Mode | Open‑Loop
Minimum | 0 | Maximum | 35940
Default | 1500 | Units |
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, BU

The speed feedback from the drive P1 position feedback interface can be used as a source to control a parameter. The speed feedback is scaled to give a value as a percentage of P1 Maximum Reference (03.043) in 0.1% units which is displayed in P1 Reference (03.045). The value is then scaled by the P1 Reference Scaling (03.044) and then routed to the destination defined by P1 Reference destination (03.046).

Normally the destination is updated every 4ms, but if the destination is the Hard Speed Reference (03.022), P1 Maximum Reference (03.043) = VM_SPEED_FREQ_REF[MAX] and P1 Reference Scaling (03.044) = 1.000 it is updated every 250μs. Although the hard speed reference is updated every 250μs internally a value in rpm or mm/s is written to Hard Speed Reference (03.022) every 4ms for indication only. It should be noted that if the fast update method is used the resolution of the speed feedback devived from the position feedback device defines the resolution of the hard speed reference and that any ripple on the feedback will be present on the hard speed reference (see Speed Feedback (03.002)).

Parameter | 03.044 P1 Reference Scaling
--- | ---
Short description | Defines the scaling applied to P1 reference
Mode | Open‑Loop
Minimum | 0.000 | Maximum | 4.000
Default | 1.000 | Units |
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 3
Coding | RW

See P1 Maximum Reference (03.043).

Parameter | 03.045 P1 Reference
--- | ---
Short description | Displays the value in P1 reference
Mode | Open‑Loop
Minimum | -100.0 | Maximum | 100.0
Default |  | Units | %
Type | 16 Bit Volatile | Update Rate | 4ms write
Display Format | Standard | Decimal Places | 1
Coding | RO, FI, ND, NC, PT

See P1 Maximum Reference (03.043).

Parameter | 03.046 P1 Reference destination
--- | ---
Short description | Defines the destination parameter for P1 reference
Mode | Open‑Loop
Minimum | 0.000 | Maximum | 59.999
Default | 0.000 | Units |
Type | 16 Bit User Save | Update Rate | Drive reset read
Display Format | Standard | Decimal Places | 3
Coding | RW, DE, PT, BU

See P1 Maximum Reference (03.043).

Parameter | 03.047 P1 SSI Incremental Mode
--- | ---
Short description | Set to 1 to enable SSI incremental mode
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

P1 Device Type (03.038): EnDat, BISS
P1 SSI Incremental Mode (03.047) has no effect and these comms modes can only operate in incremental mode, i.e. the absolute position is taken during encoder initialisation and then incremental positions are accumulated from that point on, to determine the position. If there is an error in the position read from the encoder this will be detected from the CRC check, and the position data will be ignored until correct data is available or the drive trips after a number of consecutive errors. This prevents large spurious changes in position due to data errors, and so absolute mode is not required.

P1 Device Type (03.038): SSI
If P1 SSI Incremental Mode (03.047) = 0 the complete absolute position is read at each sample. Care should be taken when using this mode as some unwanted effects can occur when the encoder passes through the boundary between its maximum position and zero. In this mode the encoder can be used for motor control provided at least 6 bits of turns information are provided by the encoder otherwise an over speed trip will be produced as the position passes over the maximum position to zero boundary. P1 Normalised Position (03.058) can be used for position control over this boundary provided the normalised turns bits are set up so that the normalised positions do not contain turns information that is not available from the encoder. As the SSI format does not include any error checking it is not possible to detect if the position data has been corrupted by noise. The benefit of using the absolute position directly from an SSI encoder is that even if the encoder communications are disturbed by noise and position errors occur, the position will always recover the correct position after the disturbance has ended.

If P1 SSI Incremental Mode (03.047) = 1 the absolute position is only taken from the encoder during initialisation. The change of position over each sample is then accumulated to determine the position. This method always gives 16 bits of turns information that can always be used without jumps in position whatever value is used as the turns bits for normalisation. If noise corrupts the data from an SSI encoder it is possible to have apparent large change of position, and this can result in the turns information becoming and remaining corrupted until the encoder is re-initialised.

If an SSI encoder is used, but is not powered from the drive, and the encoder is powered up after the drive, it is possible that the first change of position detected could be large enough to cause the problems described above. This can be avoided if the encoder interface is initialised with Initialise Position Feedback (03.075) after the encoder has powered up. If the encoder includes a power supply alarm bit, the power supply monitor should be enabled. This will ensure that the drive remains tripped until the encoder is powered up and the action of resetting the trip will reinitialise the encoder interface.

P1 Device Type (03.038): All other device types
P1 SSI Incremental Mode (03.047) has no effect.

Parameter | 03.048 P1 SSI Binary Mode
--- | ---
Short description | Set to 1 to enable SSI binary mode
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

P1 Device Type (03.038): SC SSI, SSI
SSI encoders normally use Gray code data format. However, some encoders use binary format which may be selected by setting P1 SSI Binary Mode (03.048) to one.

P1 Device Type (03.038): All other device types
P1 SSI Binary Mode (03.048) has no effect.

Parameter | 03.049 P1 Additional Power-up Delay
--- | ---
Short description | Defines an additional delay for when any attempt is made to communicate to the device P1
Mode | Open‑Loop
Minimum | 0.0 | Maximum | 25.0
Default | 0.0 | Units | s
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 1
Coding | RW, BU

When the position feedback is initialised, at power-up or at any other time, a delay is included before the information from the feedback device is used or any attempt is made to communicate with the device. The minimum delays are shown in the table below. P1 Additional Power-up Delay (03.049) defines an additional delay that is added to the minimum delay.

P1 Device Type (03.038) | Minimum delay
AB, FD, FR AB Servo, FD Servo, FR Servo SC, SC Servo Resolver, SC SC | 100ms
SC Hiperface | 150ms
EnDat, SC EnDat SSI, SC SSI BISS, SC BiSS Option Slot 1, Option Slot 2, Option Slot 3, Option Slot 4 | 1.3s

Parameter | 03.050 P1 Feedback Lock
--- | ---
Short description | Set to 1 to prevent the position feedback paramters for P1 being updated
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

If P1 Feedback Lock (03.050) = 1 then P1 Revolution/Pole Pitch Counter (03.028), P1 Position (03.029) and P1 Fine Position (03.030) are not updated. If P1 Feedback Lock (03.050) = 0 then these parameters are updated normally.

Parameter | 03.051 P1 Linear Feedback Select
--- | ---
Short description | Set to 1 to configure the P1 interface to operate with a linear position feedback device
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read, Auto-configuration write
Display Format | Standard | Decimal Places | 0
Coding | RW

If P1 Linear Feedback Select (03.051) = 0 then the drive P1 position feedback interface is configured to operate with a rotary position feedback device. P1 Rotary Turns Bits (03.033) and P1 Rotary Lines Per Revolution (03.034) should be used to set up the position feedback interface.

If P1 Linear Feedback Select (03.051) = 1 then the position feedback interface is configured to operate with a linear position feedback device. P1 Linear Comms Pitch (03.052) and P1 Linear Line Pitch (03.053) should be used to set up the position feedback interface.

Parameter | 03.052 P1 Linear Comms Pitch
--- | ---
Short description | Defines the distance covered by the least significant bit of the position information in a comms message from a linear encoder
Mode | Open‑Loop
Minimum | 0.001 | Maximum | 100.000
Default | 0.001 | Units |
Type | 32 Bit User Save | Update Rate | Background read, auto-configuration write
Display Format | Standard | Decimal Places | 3
Coding | RW

P1 Device Type (03.038): SC Hiperface, EnDat, SC EnDat, SSI, SC SSI, BiSS, SC BiSS
P1 Linear Comms Pitch (03.052) is used to define the distance covered by the least significant bit of the position information in a comms message from a linear encoder. The units used by this parameter are defined by P1 Linear Comms And Line Pitch Units (03.054).

P1 Device Type (03.038): Any other device
P1 Linear Comms Pitch (03.052) has no effect.

Parameter | 03.053 P1 Linear Line Pitch
--- | ---
Short description | Defines the linear line pitch for device P1
Mode | Open‑Loop
Minimum | 0.001 | Maximum | 100.000
Default | 0.001 | Units |
Type | 32 Bit User Save | Update Rate | Background read, auto-configuration write
Display Format | Standard | Decimal Places | 3
Coding | RW

P1 Linear Line Pitch (03.053) only has any effect if the position feedback interface is being used with a linear device (i.e. P1 Linear Feedback Select (03.051) = 1) and should be used to define the distances listed below for each type of device. The units used by this parameter are defined by P1 Linear Comms And Line Pitch Units (03.054).

P1 Device Type (03.038): AB, AB Servo
P1 Linear Line Pitch (03.053) should be set to the distance covered by one line period on the encoder.

P1 Device Type (03.038): FD, FR, FD Servo, FR Servo
P1 Linear Line Pitch (03.053) should be set to the distance covered by two line periods on the encoder.

P1 Device Type (03.038): SC, SC Hiperface, SC EnDat, SC SSI, SC Servo, SC SC, SC BiSS
P1 Linear Line Pitch (03.053) should be set to the distance covered by one sine wave period on the encoder.

P1 Device Type (03.038): Resolver
P1 Linear Line Pitch (03.053) should be set to the distance covered by one pole of the resolver divided by 214.

P1 Device Type (03.038): Any other device
P1 Linear Line Pitch (03.053) has no effect.

Parameter | 03.054 P1 Linear Comms And Line Pitch Units
--- | ---
Short description | Defines the linear units in either millimetres or micrometres
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | millimetres
1 | micrometres

P1 Linear Comms And Line Pitch Units (03.054) defines the units used by P1 Linear Comms Pitch (03.052) and P1 Linear Line Pitch (03.053) in either millimetres or micrometres.

Parameter | 03.055 P1 Pole Pitch
--- | ---
Short description | Defines the distance equivalent to one pole for linear position feedback devices
Mode | Open‑Loop
Minimum | 0.01 | Maximum | 1000.00
Default | 10.00 | Units | mm
Type | 32 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

P1 Pole Pitch (03.055) is used to define the distance equivalent to one pole for linear position feedback devices. If the linear position feedback device is being used with a linear motor, then P1 Pole Pitch (03.055) should be set to the pole pitch of the motor.

Parameter | 03.056 P1 Feedback Reverse
--- | ---
Short description | Set to 1 to reverse the direction of the position feedback
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

If P1 Feedback Reverse (03.056) = 1 the position feedback is negated. This can be used to reverse the direction of the position feedback. It should be noted that the position and the turns are negated, so for example if P1 Revolution/Pole Pitch Counter (03.028) = 0 and P1 Position (03.029) = 1000 with P1 Feedback Reverse (03.056) = 0, then if P1 Feedback Reverse (03.056) is set to one then P1 Revolution/Pole Pitch Counter (03.028) = 65535 (-1) and P1 Position (03.029) = 64536 (65536 - 1000). This will have an effect on the initial position for example, for a resolver which is a single turn absolute device, where the initial P1 Revolution/Pole Pitch Counter (03.028) = 0 with P1 Feedback Reverse (03.056) = 0 or 65535 (-1) with P1 Feedback Reverse (03.056) = 1.

Reversing the position feedback will not compensate for the following situations:

1. The direction of the incremental signals and the direction of the digital commutation signals are different for encoders which have digital commutation signals (i.e. AB Servo)
2. The direction of the SINCOS signals are incorrect for a SINCOS encoder with comms.

Parameter | 03.057 P1 Normalisation Turns
--- | ---
Short description | Defines the number of turns bits included in the normalisation parameters
Mode | Open‑Loop
Minimum | 0 | Maximum | 16
Default | 16 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

The combination of P1 Revolution/Pole Pitch Counter (03.028), P1 Position (03.029) and P1 Fine Position (03.030) give the position feedback as a 48 bit value. This position cannot be read atomically without locking the position feedback (P1 Feedback Lock (03.050) = 1) and it cannot be used directly by the Advanced Motion Controller (see Menu 31). It is useful to be able to create 32 bit position values that can be held by a single parameter as this value can be accessed atomically and can be used directly by the Advanced Motion Controller. P1 Normalisation Turns (03.057) defines the number of turns bits included in the following parameters.

P1 Normalised Position (03.058)
P1 Normalised Marker Position (03.059)
F1 Normalised Freeze Position (03.103) if P1 is the source position for freeze function F1
F2 Normalised Freeze Position (03.108) if P1 is the source position for freeze function F2

Parameter | 03.058 P1 Normalised Position
--- | ---
Short description | Displays the position taken from the position feedback device including the effect of the marker function
Mode | Open‑Loop
Minimum | -2147483648 | Maximum | 2147483647
Default |  | Units |
Type | 32 Bit Volatile | Update Rate | 250µs write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

P1 Normalised Position (03.058) is the position taken from the position feedback device including the effect of the marker function. See P1 Normalisation Turns (03.057) for details of the format.

Parameter | 03.059 P1 Normalised Marker Position
--- | ---
Short description | Displays the normalised position at the last marker event
Mode | Open‑Loop
Minimum | -2147483648 | Maximum | 2147483647
Default |  | Units |
Type | 32 Bit Volatile | Update Rate | 250µs write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

P1 Normalised Marker Position (03.059) is the value P1 Normalised Position (03.058) at the last marker event provided bit 2 of P1 Marker Mode (03.031) is set to 1. See P1 Marker Mode (03.031) for more details.

Parameter | 03.060 P1 Calculation Time
--- | ---
Short description | Defines the time from the first edge of the clock signal from the position feedback interface until the encoder has calculated the position and is ready to return this information
Mode | Open‑Loop
Minimum | 0 | Maximum | 20
Default | 5 | Units | µs
Type | 8 Bit User Save | Update Rate | Background read, auto-configuration write
Display Format | Standard | Decimal Places | 0
Coding | RW

P1 Device Type (03.038): EnDat, BiSS
P1 Calculation Time (03.060) is the time from the first edge of the clock signal from the position feedback interface until the encoder has calculated the position and is ready to return this information. This is used to calculate the overall time for a message interchange with the encoder. See P1 Low Speed Update Rate Active (03.063) for more details.

P1 Device Type (03.038): Any other type of device
P1 Calculation Time (03.060) has no effect.

Parameter | 03.061 P1 Recovery Time
--- | ---
Short description | Defines the time that must be allowed after each message interchange before a new message begins
Mode | Open‑Loop
Minimum | 4 | Maximum | 100
Default | 30 | Units | µs
Type | 8 Bit User Save | Update Rate | Background read, auto-configuration write
Display Format | Standard | Decimal Places | 0
Coding | RW

P1 Device Type (03.038): EnDat, SSI, BiSS
P1 Recovery Time (03.061) is the time that must be allowed after each message interchange before a new message begins.

P1 Device Type (03.038): Any other type of device
P1 Recovery Time (03.061) has no effect.

Parameter | 03.062 P1 Line Delay Time
--- | ---
Short description | Displays the transmission delay between the position feedback interface and the encoder and back again
Mode | Open‑Loop
Minimum | 0 | Maximum | 5000
Default |  | Units | ns
Type | 16 Bit User Save | Update Rate | Background read, position feedback initialisation write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

P1 Device Type (03.038): EnDat, SC EnDat, BiSS, SC BiSS
During position feedback initialisation the transmission delay between the position feedback interface and the encoder and back again is measured and stored in P1 Line Delay Time (03.062). This value is then used to compensate for this delay so that the clock/data skew does not prevent the data from the encoder from being read. This means that longer line lengths can be used with these feedback devices provided the correct cable and connection arrangements are used.

P1 Device Type (03.038): Any other type of device
P1 Line Delay Time (03.062) is always zero.

Parameter | 03.063 P1 Low Speed Update Rate Active
--- | ---
Short description | Indicates when the low speed update rate is active
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

P1 Device Type (03.038): EnDat, SSI, BISS
There is a delay when the position information is obtained via a communications interface from an encoder. It is assumed that the position information is taken from all types of encoder at a fixed datum point during each sample period. The drive initiates the comms transfer at a suitable point in advance of the datum to ensure that the position information is available when required. A correction is then applied to the position information based on the change of position over the previous sample and the advance time so that the position appears to have been sampled at the datum. If the communications exchange, including allowing the encoder a recovery time (P1 Recovery Time (03.061)), is completed in 60μs and the time required to obtain the full position is completed in 40μs then the position is sampled at each current controller task and P1 Low Speed Update Rate Active (03.063) = 0. Otherwise if the communication exchange is completed in 230μs the position is sampled every 250μs and P1 Low Speed Update Rate Active (03.063) = 1. If the complete exchange takes any longer an Encoder 8 trip is initiated. The following table shows the calculations used by the drive to determine the necessary time to obtain the required data.

Protocol | Time for full position | Time for complete data exchange
Endat 2.1 encoder | tST + tD + 10T + 2T + NtT + 5T where tcal ≤ tST + tD/2+ 10T tST + tD + tcal + 2T + NtT + 5T where tcal > tST + tD/2 + 10T | Time for full position + tm
EnDat 2.2 encoder | tST + tD + 10T + 3T + NtT + 5T + tAdd where tcal ≤ tST + tD/2+ 10T tST + tD + tcal + 3T + NtT + 5T + tAdd where tcal > tST + tD/2 + 10T | Time for full position + tm
BiSS | tD + tcal + 2T + NtT + 2T + (CRCBits x T) | Time for full position + tm
SSI | tD + T + NtT (tD cannot be measured, and so a value of 1.25μs is used) | Time for full position + tm

where

Value | Description | Source
tST | EnDat start time | For 100K baud = 5us, 200K baud = 2.5us, for all other baud rates = 2μs
tD | Transmission delay from the drive to the encoder and back | P1 Line Delay Time (03.062)
T | 1 / baud rate | P1 Comms Baud Rate (03.037)
tcal | Position calculation time | P1 Calculation Time (03.060)
Nt | Total number of position information bits | P1 Comms Bits (03.035)
tm | Encoder recovery time | P1 Recovery Time (03.061)
tAdd | Time for additional information | tAdd1 = 31T + tST + 30T
CRCBits | The number of bits in the CRC applied to the position | P1 Additional Configuration (03.074)

P1 Device Type (03.038): Option Slot 1, Option Slot 2, Option Slot 3, Option Slot 4
It is intended that position information is provided by an option module with an upate rate of 250us. It is assumed that the position that is provided is sampled 230us before the position datum point. P1 Low Speed Update Rate Active (03.063) is always one to indicate that a sample rate of 250us is being used.

P1 Device Type (03.038): Any other type of device
P1 Low Speed Update Rate Active (03.063) is always zero.

Parameter | 03.064 P1 Encoder Protocol Detected
--- | ---
Short description | Defines which protocol is used with the device P1
Mode | Open‑Loop
Minimum | 0 | Maximum | 4
Default |  | Units |
Type | 8 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, TE, ND, NC, PT

Value | Text
0 | None
1 | Hiperface
2 | EnDat2.1
3 | EnDat2.2
4 | BiSS

P1 Encoder Protocol Detected (03.064) shows the encoder comms protocol detected during position feedback initialisation. If P1 Device Type (03.038) is set to SC Hiperface or BiSS then P1 Encoder Protocol Detected (03.064) is set to the appropriate value after successful communication with the encoder during initialisation. If P1 Device Type (03.038) is set to EnDat or SC EnDat then P1 Encoder Protocol Detected (03.064) is set to the appropriate EnDat protocol after successful communication with the encoder during initialisation. If communications is not successful during initialisation then P1 Encoder Protocol Detected (03.064) is set to 0.

Parameter | 03.065 P1 Resolver Poles
--- | ---
Short description | Defines the number of poles for the resolver connected to P1
Mode | Open‑Loop
Minimum | 1 | Maximum | 10
Default | 1 | Units | PolePairs
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

P1 Device Type (03.038): Resolver
P1 Resolver Poles (03.065) should be set to the number pole pairs for the resolver connected to the P1 position feedback interface. If the resolver is being used for motor control then a 2 pole resolver can be used with any motor, but if the number of resolver poles is greater than 2, it can only be used when motor poles / resolver poles is an integer (i.e. a 4 pole resolver can be used with an 8 pole motor). Note that this value is only used if P1 Linear Feedback Select (03.051) = 0. If not then the position feedback must be set up using P1 Linear Line Pitch (03.053) and P1 Pole Pitch (03.055).

P1 Device Type (03.038): Any other type of device
P1 Resolver Poles (03.065) has no effect.

Parameter | 03.066 P1 Resolver Excitation
--- | ---
Short description | Defines the excitation of the resolver when connected to P1
Mode | Open‑Loop
Minimum | 0 | Maximum | 7
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | 6kHz 3V
1 | 8kHz 3V
2 | 6kHz 2V
3 | 8kHz 2V
4 | 6kHz 3V Fast
5 | 8kHz 3V Fast
6 | 6kHz 2V Fast
7 | 8kHz 2V Fast

P1 Device Type (03.038): Resolver
P1 Resolver Excitation (03.066) defines the excitation voltage and frequency. A level of 3V r.m.s. should be used with 3:1 resolvers and 2V r.m.s. with 2:1 resolvers. These give a nominal level of 1V r.m.s. feedback into the position feedback interface. Other ratios can be used, but if the feedback is increased above the expected levels the feedback seen by the drive will be distorted. The resolution of the position feedback will be reduced if the feedback is less than 1V r.m.s. With a 2 pole resolver the nominal resolution is equivalent to 1600 line encoder. If the number of resolver poles are increased then the resolution increases, for example a 4 pole resolver gives a resolution equivalent to a 3200 line encoder, etc. The position feedback system allows for a delay from the excitation to the feedback from the resolver of up to 45o and will compensate for this lag during the position feedback initialisation process. (It should be noted that the excitation voltage given is the nominal level, but this can slightly higher than the nominal level.)

The resolver interface offers two sampling rates: standard and fast. With standard sampling (P1 Resolver Excitation (03.066) < 4) any switching frequency can be used with any resolver excitation frequency and the switching frequency can be changed when the position feedback is being used without any transient effects. There is a 250us sampling delay with this system and if the resolver feedback is used for motor control the system can become unstable at high speeds. It is recommended that the motor speed is limited to 9000rpm / Motor Pole Pairs. With fast sampling (P1 Resolver Excitation (03.066) ≥ 4) the sample delay is significantly reduced and resolver feedback can be used up to the maximum limit of 30000rpm, but the feedback is much noisier and the acoustic noise produced by the motor is increased. It is possible to switch between standard and fast sampling while the drive is enabled and controlling a motor, so for example standard sampling can be used at low speeds, and then fast sampling can be used at higher speeds. Normally when P1 Resolver Excitation (03.066) is changed an Encoder 7 is initiated because the position feedback set-up has been changed and the position feedback interface needs to be re-initialised. However, if the new value of P1 Resolver Excitation (03.066) is the old value plus or minus 4 (i.e. 0 to 4, or 5 to 1, etc.) then a trip is not initiated and the interface does not need to be initialised.

The following restrictions apply if fast sampling is selected:

1. 2, 4, 8 or 16kHz switching frequencies should be used with 8kHz excitation. 3, 6 or 12kHz switching frequencies should be used with 6kHz excitation. If these conditions are not met the system will automatically operate with standard sampling.
2. If the switching frequency is changed by one step, i.e. from 2 to 3kHz, there will be a transient in the position feedback. To ensure that this does not happen as the drive alters the switching frequency because it has become too hot Auto-switching Frequency Step Size (05.036) should be left at its default value, so that all changes are made in steps of 2.
3. If the resolver feedback is not being used as the feedback for motor control then its sample rate is automatically reduced and the position feedback will automatically operate with standard sampling.
4. If a linear mode is selected (i.e. P1 Linear Feedback Select (03.051) = 1) then the system will operate with standard sampling.

P1 Device Type (03.038): Any other type of device
P1 Resolver Excitation (03.066) has no effect

Parameter | 03.067 P1 User Comms Enable
--- | ---
Short description | Enables the use of the user comms paramters to communicate to the encoder connected to P1
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 8 Bit Volatile | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, NC, PT

If P1 User Comms Enable (03.067) set to one it is possible to use P1 User Comms Transmit Register (03.068) and P1 User Comms Receive Register (03.069) to communicate with an encoder that has a Hiperface, EnDat 2.1, EnDat2.2 or BiSS interface. A description of how to use these registers is given below.

P1 Device Type (03.038): SC Hiperface, SC EnDat
Hiperface or EnDat 2.1 communications are used as appropriate if P1 User Comms Enable (03.067) is set to one.

P1 Device Type (03.038): EnDat
Communication is enabled when P1 User Comms Enable (03.067) is set to one. If the encoder supports EnDat 2.2 it is possible to enable user communications at any time even if the drive is enabled. Otherwise if the encoder only supports EnDat 2.1 communication with the encoder is not possible.

P1 Device Type (03.038): BISS, SC BiSS
If P1 User Comms Enable (03.067) is set to one it is possible to enable user communications at any time even if the drive is enabled.

Encoder communications
A communication channel is provided to allow the user to communicate with an encoder connected to one of the communications interfaces. It should be noted that the communications channel is disabled under the following conditions:

1. If auto-configuration is active.
2. During the transfer of electronic nameplate data.
3. If the position feedback device is not initialised.
4. The channel is being used by an option module with safety functions.

To send a message to the encoder the required message must be written to the transmit register. To read the response from the encoder the data is read from the receive register. The data is written one byte at a time and is stored in a 16 byte buffer before being sent to the encoder. The data should only be written to the transmit register when it has been cleared to zero by the drive. Bits 13 to 15 are used to control the interface.

Bit | Function
15 | This bit should be set to one each time data is written to the transmit register. This indicates that data has been written. This bit will be cleared when the LS byte of the data has been transferred into the comms buffer.
14 | This bit should be set when the last byte of the message is written to the transmit register. The data will be read and transferred to the comms buffer and then the message will be sent to the encoder.
13 | This bit should be set when the first byte of the message is written to the transmit register. Setting this bit will reset the pointer to the start of the comms buffer.

Data can be read from the receive register at any time. If there is data in the buffer bit 15 will be set. Once the data has been read the register should be cleared and the drive will transfer the next byte of data to the register.

Bit | Function
15 | Indicates that data from the last transfer can be read from the receive register.
14 | Indicates that the last byte from the receive message is in the register.
13 | There is no data in the receive buffer and the LS byte of the receive register is the comms system status. If there was an error in the received message one of the status error bits will also be set until the comms is used again by this system or by the drive.

The status flags are defined as follows:

Bit | Meaning
0 | The number of bytes put into the transmit buffer is not consistent with the expected message length. (Hiperface only)
1 | The number of bytes written to the transmit buffer, or the expected length of the store data transmit message, or the expected length of a read data message have exceed the length of the buffer. (Hiperface only)
2 | The command code is not supported.
3 | A valid response was not received from the encoder.

The following sequence should be followed when transmitting and receiving data to ensure that the received data is always read correctly.

1. Check that P1 User Comms Receive Register (03.069) is not zero.
2. Check that P1 User Comms Transmit Register (03.068) is zero.
3. Write each word of the transmit message to P1 User Comms Transmit Register (03.068) in turn, waiting each time for the drive to return P1 User Comms Transmit Register (03.068) back to zero before writing the next word.
4. Write zero to P1 User Comms Receive Register (03.069).
5. Read P1 User Comms Receive Register (03.069) and when it is not zero the drive has updated it with a receive word.
6. Read each receive word in turn writing zero to P1 User Comms Receive Register (03.069) after reading the word.

If the above sequence is not followed correctly, it is possible that data from the transmit message will be seen in the first read of the receive message. It is not essential that any or all of the receive message is read before sending a new transmit message, and so steps 4 to 6 can be omitted if required provided step 1 is not ignored.

Hiperface
Up to 15 bytes of data can be written to the buffer. The first byte should be the encoder address. The checksum will be calculated by the drive and added to the end of the message before the message is transmitted to the encoder. The drive checks the checksum of the received message. If successfully received, the receive message can be read via the receive register including the address and the checksum received from the encoder. It should be noted that the encoder must be set up for 9600 baud, 1 start bit, 1 stop bit and even parity (default set-up) for the encoder comms to operate with the drive. Also the data block security should not be enabled in the encoder if the drive encoder nameplate system is to operate correctly. See Hiperface specification for more details of the comms message format.

The following commands are supported:

Code | Command
0x42 | Read position
0x43 | Set position
0x44 | Read analog value
0x46 | Read counter
0x47 | Increment counter
0x49 | Clear counter
0x4a | Read data (maximum of 10 bytes)
0x4b | Store data (maximum of 9 bytes)
0x4c | Data field status
0x4d | Create a data field
0x4e | Available memory
0x50 | Read encoder status
0x52 | Read type
0x53 | Reset encoder

SC EnDat
Up to 4 bytes can be written to the buffer in the following format.

Byte 0 |  |  |
Command | Address | Data (MSB) | Data (LSB)

The following commands are supported.

Code | Command | Address | Data (MSB) | Data (LSB)
0x07 | Encoder to send position value | Any | Any | Any
0x0E | Selection of memory area | MRS code | Any | Any
0x1C | Encoder to receive parameter | Address | Data (MSB) | Data (LSB)
0x23 | Encoder to send parameter | Address | Any | Any
0x2A | Encoder to receive reset | Any | Any | Any

The message from the encoder contains a CRC which is checked. If there are no errors in the message, then the message is put into the comms buffer. The position is retrieved from the drive buffer most significant byte first (Byte 0) and least significant byte last (Byte 7). An example is shown below where a 48 bit value has been read from the encoder which contains an error bit (Bit 0) and 47 bits of position data (Bits 1 to 47) where Bit 1 is the least signficant bit of the position. If there are less position bits the position is right justified with leading zeros.

Byte 0 |  |  |  |  |  |  | Byte 7
0 | 0 | Bits47-40 | Bits 39-32 | Bits 31-24 | Bits 23-16 | Bits 15-8 | Bits 7-0

If any other command is sent the response is shown below. The response is available when the encoder has responded, but for "Encoder to recieve parameter" and "Encoder to receive reset" commands there is an additional delay of 12ms and 20ms respectively to allow the encoder to be ready again.

Byte 0 |  | Byte 2
Address | Data (MSB) | Data (LSB)

EnDat
Up to 4 bytes can be written to the buffer in the same format as for EnDat 2.1. The following commands are supported.

Code | Command | Address | Data (MSB) | Data (LSB)
0x09 | Encoder to send position value with additional information and select memory area | MRS code | 0x00 | Block address
0x1B | Encoder to send position value with additional information and receive parameters | Address | Data (MSB) | Data (LSB)
0x24 | Encoder to send position value with additional information and send parameters | Address | Any | Any
0x2D | Encoder to send position value with additional information and receive error reset | Any | Any | Any
0x36 | Encoder to send position values and receive test command | Any | Any | Any

The message from the encoder contains a CRC which is checked. If there are no errors in the message the message is put into the comms buffer.

Byte 0 |  | Byte 2
Additional information 1 Byte 0 (B7) WRN (B6) RM (B5) Busy (B4) I4 (B3) I3 (B2) I2 (B1) I1 (B0) I0 | Additional Information 1 Byte 1 | Additional Information 1 Byte 2

It should be noted that the encoder is set up automatically so that it always returns Additional Information 1 with no data contents. An MRS is sent to the encoder to select which data contents should be included in Additional Information 1. An MRS code can also be used to select Additional Information 1, Additional Information 2 or no Additional Information to be sent from the encoder, but these commands must not be used. Although the contents of Additional Information 1 can be changed the encoder should always be in the state where it transmits only Additional Information 1.

BiSS, SC BiSS
It is possible to read or write to 8 bit registers in a BiSS device. The addressing range is 0 to 127 giving access to 128 registers. Two bytes should be written to the buffer for both read or write operations. Byte 0 contains the command in bit 7 (0 = read, 1= write) and the register address in bit 6 to bit 0. For reading Byte 1 can contain any value, for writing it should contain the data to be written.

Byte 0 | Byte 1
Command + Address | Data

The response is always two bytes as shown below. Byte 0 is the same as Byte 0 in the request sent to the drive. For reading Byte 1 is the value read from the register and for writing it is always zero.

Byte 0 | Byte 1
Command + Address | Data

Parameter | 03.068 P1 User Comms Transmit Register
--- | ---
Short description | Defines the value present in the user comms transmit register
Mode | Open‑Loop
Minimum | 0 | Maximum | 65535
Default | 0 | Units |
Type | 16 Bit Volatile | Update Rate | Background read/write
Display Format | Standard | Decimal Places | 0
Coding | RW, NC, PT, BU

See P1 User Comms Enable (03.067).

Parameter | 03.069 P1 User Comms Receive Register
--- | ---
Short description | Defines the value present in the user comms receive register
Mode | Open‑Loop
Minimum | 0 | Maximum | 65535
Default | 0 | Units |
Type | 16 Bit Volatile | Update Rate | Background read/write
Display Format | Standard | Decimal Places | 0
Coding | RW, NC, PT, BU

See P1 User Comms Enable (03.067).

Parameter | 03.070 P1 Position Feedback Signals
--- | ---
Short description | Shows the state of the signals from the position feedback device
Mode | Open‑Loop
Minimum | 0 (Display: 000000) | Maximum | 63 (Display: 111111)
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Binary | Decimal Places | 0
Coding | RO, ND, NC, PT

P1 Position Feedback Signals (03.070) shows the state of the signals from the position feedback device as given in the table below where the signals are relevant for the type of device. P1 Position Feedback Signals (03.070) is only intended as a debugging aid.

P1 Position Feedback Signals (03.070) bits | Signals
0 | A or F or Cos
1 | B or D or R or Sin
2 | Z
3 | U
4 | V
5 | W

For Cos and Sin signals the relevant bits of P1 Position Feedback Signals (03.070) will be set when the signals are positive and cleared when the signals are negative.

Parameter | 03.071 P1 Error Detected
--- | ---
Short description | Indicates if an error has been detected with the position feedback device connected to the P1 position interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

P1 Error Detected (03.071) is set if an error has been detected with the position feedback device connected to the P1 position interface. This parameter is useful if encoder trips have been disabled by setting bit 3 of P1 Error Detection Level (03.040). It should be noted that this bit is not set if specific trips are disabled with bits 0 to 2 of P1 Error Detection Level (03.040).

Parameter | 03.073 P1 Absolute Turns Recovery Enable
--- | ---
Short description | Set to 1 to allow turns information beyond the number of turns bits provided by the position feedback device connected to P1 to be stored on power-down and recovered at next power-up
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background Read
Display Format | Standard | Decimal Places | 0
Coding | RW

P1 Absolute Turns Recovery Enable (03.073) can be used to remove the masking applied to P1 Revolution/Pole Pitch Counter (03.028) for any type of position feedback device. If P1 Device Type (03.038) is set to EnDat, SC.EnDat, SC.Hiperface, SSI, SC.SSI, BiSS, Option Slot 1, Option Slot 2, Option Slot 3 or Option Slot 4 then this parameter has an additional feature which allows turns bits beyond the number of turns bits provided by the position feedback device to be stored on power-down and then recovered on the next power-up. P1 Revolution/Pole Pitch Counter (03.028) is saved as a power-down save parameter. If P1 Absolute Turns Recovery Enable (03.073) = 0 the value saved at power-down is ignored on the next power-up and P1 Revolution/Pole Pitch Counter (03.028) is set up based on the information provided by the position feedback device. For example a device with 12 turns bits can define the position with up to 4096 turns. If P1 Absolute Turns Recovery Enable (03.073) = 1 the turns beyond those provide by the position feedback device are simulated from the saved value. This means that 65536 turns can be generated from a position feedback device with any number of turns bits. The following should be noted:

1. If the position feedback device moves by more than +/-1/4 of the range of the most significant turns bit while powered down the turns at power-up will not be correct. For example a device with 12 turns bits must not move by more than the range defined by 10 turns bits, or a device with no turns bits must not move by more than 1/4 of a turn.
2. This feature is not applicable to linear position feedback devices.
3. If an SSI based device is being used then P1 SSI Incremental Mode (03.047) must be set to one.
4. The recovered turns bits are stored in P1 Revolution/Pole Pitch Counter (03.028). To reset the additional bits P1 Absolute Turns Recovery Enable (03.073) should be set to zero to remove the recovered turns bits. A parameter save should then be initiated using a value of 1 or 1001 in parameter mm.000 to save the contents of P1 Revolution/Pole Pitch Counter (03.028). Absolute turns recovery can then be selected again by setting P1 Absolute Turns Recovery Enable (03.073) to one.
5. Absolute turns recovery is not possible when Low Under Voltage Threshold Select (06.067) = 1 or Backup Supply Mode Enable (06.068) = 1 or User Supply Select (06.072) = 1. If absolute turns recovery is required when one of these modes is enabled then a user save (Parameter mm.000 (mm.000) = 1 or 1001) should be performed before the drive is powered down.

Parameter | 03.074 P1 Additional Configuration
--- | ---
Short description | Provides additional configuration information for the position feedback device not included in the other set-up parameters.
Mode | Open‑Loop
Minimum | 0 | Maximum | 511116116
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

P1 Additional Configuration (03.074) provides configuration information, not covered by the other set-up parameters, for the position feedback device connected to the P1 position feedback interface and is specific to the type of device being used.

P1 Device Type (03.038): BiSS, SC BiSS

This parameter is split into 3 fields as shown below.

Decimal Digits | 9-6 | 5-3 | 2-0
| CRC polynomial | Rotary Turns Padding | Rotary Position Padding
Default | 0067 | 000 | 000

CRC polynomial
The CRC polynomial is a bit representation of the terms of a polynomial used to generate the CRC applied to the position and the additional data transferred to/from the encoder via the BiSS communications channel. The standard value is 0067 which in hexadecimal is 0x0043, or in binary form is 0000 0000 0100 0011. The bits that are set to one show which terms exist in the polynomial. The standard value has bits 6, 1 and 0 set to one and gives the polynomial normally used with BiSS encoders which is X6+X1+1. If the encoder uses a different polynomial then this can be selected with the four digits (9-6). The maximum value is 511 (0x01FF), and so a polynomial up to degree 10 can be set up.

Rotary Turns Padding and Rotary Position Padding
The turns, and position within a turn, provided by a rotary encoder may not completely fill the number of bits provided. The unfilled bits will be padded with zeros. The total number of bits provided for the turns including zero padding is given by P1 Rotary Turns Bits (03.033). The zero padding is given by decimal digits 5 to 3 of P1 Additional Configuration (03.074). Digits 4 and 3 give the number of bits and digit 5 specifies whether the padding is on the left (0) or on the right (1). For example a value of 104 would specify 4 padding bits on the right of the turns data. The default value of 000 specifies no padding. If the padding value is outside the range +/-16 then an Encoder 14 is initiated. The total number of bits provided for position within a turn is given by P1 Comms Bits (03.035) - P1 Rotary Turns Bits (03.033). The zero padding is given by decimal digits 2 to 0 of P1 Additional Configuration (03.074) in the same manner as is used for the turns padding. It is not possible to specify zero padding for linear encoders.

P1 Device Type (03.038): Any other device type
This parameter has no effect.

Parameter | 03.075 Initialise Position Feedback
--- | ---
Short description | Set to 1 to re-initialise any position feedback device connected
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit Volatile | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, NC

If Initialise Position Feedback (03.075) is set to one any position feedback devices connected to the drive position feedback interfaces or any position feedback category option modules will be re-initialised.

Parameter | 03.076 Position Feedback Initialized
--- | ---
Short description | Indicates the initialisation state of position feedback devices connected
Mode | Open‑Loop
Minimum | 0 (Display: 0000000000) | Maximum | 1023 (Display: 1111111111)
Default | 0 (Display: 0000000000) | Units |
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Binary | Decimal Places | 0
Coding | RO, NC, PT

Position Feedback Initialized (03.076) contains flags that represent the initialisation state of position feedback devices connected to the drive position feedback interfaces or position feedback interfaces on position feedback category option modules. One indicates that the interface is initialised and zero indicates that the interface is not initialised. The flags are assigned as shown below.

Bit | Position feedback interface
0 | P1 Drive
1 | P2 Drive
2 | P1 Option slot 1
3 | P2 Option slot 1
4 | P1 Option slot 2
5 | P2 Option slot 2
6 | P1 Option slot 3
7 | P2 Option slot 3
8 | P1 Option slot 4
9 | P2 Option slot 4

If no option module, or an option module other than a position feedback category module, is fitted in an option slot then the relevant flag is always set to one. If an attempt is made to enable the drive when any of the flags are zero the drive initiates an Encoder 7 trip. If a drive reset is initiated, the bits in Position Feedback Initialized (03.076) are checked, and if any position feedback devices are not initialised an attempt is made to initialise them.

The table below shows the initialisation process for different position feedback devices that can be connected to the drive.

Encoder types | Initialisation process
AB, FD, FR Resolver | None. Initialisation is immediate and is always successful. The position feedback is set to zero on initialisation.
AB Servo FD Servo FR Servo SC Servo | The absolute position used to control a motor can only be defined accurately after two different changes of state of the UVW commutation signals. Initialisation resets the system that ensures that the UVW signals alone will be used to define the motor position until the encoder has moved through two valid commutation signal state changes. Initialisation is immediate and is always successful. The position feedback is set to zero on initialisation.
SC | The SINCOS interpolation system must be initialised. Initialisation is immediate and is always successful. The position feedback is set to zero on initialisation.
SC Hiperface SC EnDat SC SSI | Auto-configuration if required except SC SSI. The absolute position must be obtained via comms. This may cause a large change in position feedback. The SINCOS interpolation system must be initialised. This may have a small effect on the position feedback.
EnDat BiSS SSI | Auto-configuration if required except SSI. The absolute position must be obtained via comms. This may cause a large change in position feedback.
SC SC | The absolute position used to control a motor is obtained from the sine and cosine signals provided for one revolution until the marker pulse occurs. The position obtained from the marker pulse is assumed to be a position of zero. Once a marker has occurred the incremental position is used and the single turn sine wave signals are ignored. When the position feedback device is initialised the single turn sine wave signals are used again until another marker event occurs. No part of the initialisation process affects the position feedback seen in parameters, except that the SINCOS interpolation system must be initialised which may have a small effect on the position feedback. Initialisation is immediate and is always successful.

Parameter | 03.085 Encoder Simulation Source
--- | ---
Short description | Defines the source parameter used for the encoder simulation
Mode | Open‑Loop
Minimum | 0.000 | Maximum | 59.999
Default | 3.016 | Units |
Type | 16 Bit User Save | Update Rate | Reset read
Display Format | Standard | Decimal Places | 3
Coding | RW, PT, BU

Encoder Simulation Source (03.085) is used to select a parameter as the input to the encoder simulation system. If Encoder Simulation Source (03.085) is zero then no source is selected and the encoder simulation system is disabled. The encoder simulation output connections are shared with the P1 and P2 position feedback interfaces, and so encoder simulation may be disabled because the connections are not available. See Encoder Simulation Status (03.086) for details.

Any parameter can be selected as the source, but it is assumed that the input is a 16 bit value with a range from 0 to 65535 or from -32768 to 32767. The source parameter is treated differently depending on the value of Encoder Simulation Mode (03.088) as given in the table below.

Encoder Simulation Mode (03.088) |
Hardware (0) | Encoder Simulation Source (03.085) must be set to 3.029 for the output to be enabled and the position from the P1 position feedback interface is used and P1 Position (03.029) is the source.
Lines Per Rev (1) or Ratio (2) | If Encoder Simulation Source (03.085) = 3.029 (i.e. P1 Position (03.029) is the source) then P1 Position (03.029) and P1 Fine Position (03.030) are combined as a 16 bit value with 16 bit fractional part as the input to the encoder simulation system, which gives additional output resolution if encoder simulation ratio is greater than unity. The encoder simulation system is intended to be used with a 16 bit source parameter. If the source of the encoder simulation system is not a 16 bit parameter then the drive uses the source parameter as follows. 1 bit parameter: Zero extended 8 bit parameter: Sign extended if BU attribute is zero (signed), otherwise zero extended (unsigned) 32 bit parameter: Only the least significant word is used.
SSI (3) | For SSI output mode the number of bits included in the output can be selected (see Encoder Simulation Mode (03.088) for details).

Although Encoder Simulation Source (03.085) is not a standard source parameter in common with other sources the actual source is only changed on drive reset.

Parameter | 03.086 Encoder Simulation Status
--- | ---
Short description | Displays the status of the encoder simulation
Mode | Open‑Loop
Minimum | 0 | Maximum | 2
Default |  | Units |
Type | 8 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, TE, ND, NC, PT

Value | Text
0 | None
1 | Full
2 | No Marker Pulse

The availability of the encoder simulation output on the 15 way connector on the drive is dependent on the type of feedback device selected with P1 Device Type (03.038). Priority is as follows from highest to lowest priority:

1. P1 position feedback interface
2. Encoder simulation output
3. P2 position feedback interface

Encoder Simulation Status (03.086) shows the status of the encoder simulation output.

0: None
The encoder simulation output is not enabled or is not available.

1: Full
Full encoder simulation with marker output is available.

2: No Marker
Encoder simulation without marker output is available.

Parameter | 03.087 Encoder Simulation Sample Period
--- | ---
Short description | Defines the sample period of the encoder simulation
Mode | Open‑Loop
Minimum | 0 | Maximum | 3
Default | 2 | Units | ms
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | 0.25
1 | 1
2 | 4
3 | 16

The update rate of the encoder simulation system is nominally 250μs, i.e. default value of Encoder Simulation Sample Period (03.087), but if the update rate of the source parameter is different, the encoder simulation output will consist of bursts of pulses at the update rate of the parameter. To prevent this and to give a smooth output, the update rate can be adjusted with Encoder Simulation Sample Period (03.087). Encoder Simulation Sample Period (03.087) has no effect if hardware mode is selected, i.e. Encoder Simulation Mode (03.088) = 0.

Parameter | 03.088 Encoder Simulation Mode
--- | ---
Short description | Defines the mode of the encoder simulation
Mode | Open‑Loop
Minimum | 0 | Maximum | 3
Default | 1 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Hardware
1 | Lines Per Rev
2 | Ratio
3 | SSI

Encoder Simulation Mode (03.088) defines the encoder simulation output as incremental signals (AB, FD or FR) derived directly via hardware, incremental signals generated via software or SSI data generated via software.

0: Hardware
The encoder simulation output is derived directly in hardware from the P1 position feedback interface in the drive and the output is derived from the input with negligible delay. The ratio between the input at the P1 interface and the output is either unity or a limited number of binary divider ratios (see Encoder Simulation Hardware Divider (03.089)). Hardware mode only produces an output with AB, FD, FR, SC, SC Hiperface, SC EnDat or SC SSI type devices. It should be noted that with a SINCOS source device the output is based on the zero crossings of the sine wave inputs and does not include interpolation. If Encoder Simulation Hardware Marker Lock (03.090) = 0 the marker output is derived directly from the marker input. If Encoder Simulation Hardware Marker Lock (03.090) = 1 the incremental output signals are adjusted on each marker event so that the A and B are high with an AB type output, or F is high with an FD or FR type output. Marker locking is not recommended if the number of lines per revolution of the encoder simulation source combined with the ratio does not give an encoder simulation output with a multiple of 4 counts per revolution (i.e. between each output marker event) for AB signals, or a multiple of 2 counts for FD or FR signals, because this causes a count error in the system receiving these signals. The input marker pulse width is not adjusted to take account of the divider ratio, but is simply routed from the input to the output. Therefore the output marker pulse becomes shorter with respect to the output incremental signals as the divider ratio is increased.

1: Lines Per Rev
The encoder simulation output is derived via software from the selected source with a resolution defined by Encoder Simulation Output Lines Per Revolution (03.092) with a minimum delay of 250μs which may be extended if Encoder Simulation Sample Period (03.087) is set up for a longer sample period. Note that the number of output lines per revolution apply to a quadrature (AB) type device, and that if FD or FR mode are selected the number of lines per revolution are 2 x Encoder Simulation Output Lines Per Revolution (03.092). The output is derived by applying a ratio and output counter roll-over limit defined by Encoder Simulation Output Lines Per Revolution (03.092) as shown below. The output marker is produced when the output counter is zero.

If P1 Position (03.029) is selected as the source and Encoder Simulation Incremental Mode Select (03.091) = 0 then the input and output counters are synchronised at power-up and when the P1 position feedback interface becomes initialised, so that the output marker is synchronised with zero position for the P1 position feedback interface. For devices that support a marker, the effect of the marker on the position can be selected using P1 Marker Mode (03.031). At power-up and on device initialisation there will be a step change in position from zero to the actual position from the device and the pulses necessary to make this change are produced at the encoder simulation output. If a marker event occurs that causes a step change in position, again the necessary pulses will be produced for this change of position. Where large sudden changes occur the maximum output frequency is limited to 500kHz, and so it may take some time for the output position to reach the input position. This mode of operation gives an initial position change from zero position and then follows all changes of position from that point onwards, and may be used to follow the absolute position of the device connected to the P1 position feedback interface.

If P1 Position (03.029) is selected as the source and Encoder Simulation Incremental Mode Select (03.091) = 1 then the encoder simulation output only follows the changes of source position. At power-up, on device initialisation and a marker event no additional pulses are produced to give the absolute position of the device related to zero position. The encoder simulation output markers is not synchronised to the source marker.

If a source other than P1 Position (03.029) is selected Encoder Simulation Incremental Mode Select (03.091) has no effect and the encoder simulation system always operates in absolute mode.

2: Ratio
The encoder simulation is derived in the same way as described previously for Encoder Simulation Mode (03.088) = 1 (i.e. lines per rev mode), except that different parameters are used to set up the system giving more flexibility as shown below.

With the default settings (Encoder Simulation Numerator (03.093) = 65536, Encoder Simulation Denominator (03.094) = 65536 and Encoder Simulation Output Roll-over Limit (03.095) = 65535) the output produces a state change each time the source parameter changes by one. The numerator and denominator can be changed to provide a different ratio between the source and the output. Output markers are produced each time the output counter is zero and the counters are synchronised in the same way as for lines per rev mode. It is possible to control the roll-over limit of the output counter and hence the rate at which output markers are produced using Encoder Simulation Output Roll-over Limit (03.095). For example if the ratio is set to 1024/ 65536 and the roll-over limit is 1023 then one output marker is produced for every 1024 lines of output incremental signals. If the roll-over limit is changed to 512, then two output markers are produced for every 1024 lines of output incremental signals.

3: SSI
In this mode the B output becomes the clock input and the A output is the data output. If the source position is the P1 position feedback interface the data from the position feedback interface is transferred to the SSI output register once per sample period defined by Encoder Simulation Sample Period (03.087). An example is given below which shows how the data is aligned.

The SSI output is then clocked out from the register as shown in another example below which includes 15 bits of data.

It should be noted that the data is shifted out by a clock that is produced by the SSI master connected to the encoder simulation interface as the interface is emulating an SSI encoder. However, unlike an SSI encoder the position data is not sampled on the first edge of the clock, but is updated by the drive at the rate defined by Encoder Simulation Sample Period (03.087). If the P1 position interface is being used as the source the power supply alarm bit (PS) is the inverse of the initialised flag in Position Feedback Initialized (03.076) related to this interface. The master can clock out as many bits of data as required, but once the power supply alarm bit has been produced the output will remain low. The SSI interface reset time (tm) of 20μs is required so that the interface can detect the end of the transmission and reset itself so that the output data begins again at the most significant bit. During this period the master should hold the clock line high. The master should not use a clock frequency of less than 50kHz or else spurious reset periods may be detected.

If any other parameter is used as the source the most significant M bits of the source parameter are used, where M = Encoder Simulation SSI Comms Bits (03.097) - 1. If the source parameter has less than M bits then trailing zeros are added. The power supply alarm bit is always zero in this mode.

Parameter | 03.089 Encoder Simulation Hardware Divider
--- | ---
Short description | Defines the divider ratio between the device connected to the P1 interface and the encoder simulation output when hardware simulation mode is used
Mode | Open‑Loop
Minimum | 0 | Maximum | 7
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

If hardware mode is selected (i.e. Encoder Simulation Mode (03.088) = 0) then Encoder Simulation Hardware Divider (03.089) defines the divider ratio between the device connected to the P1 position feedback interface and the output as 1/2Encoder Simulation Hardware Divider (03.089). The maximum allowed input frequency is 500kHz, and so the maximum output frequency with the highest ratio of unity is 500kHz.

Parameter | 03.090 Encoder Simulation Hardware Marker Lock
--- | ---
Short description | Defines if the marker output is derived directly from the marker input
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See Encoder Simulation Mode (03.088).

Parameter | 03.091 Encoder Simulation Incremental Mode Select
--- | ---
Short description | Set to 1 to select incremental mode for the encoder simulation
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 1 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, BU

See Encoder Simulation Mode (03.088).

Parameter | 03.092 Encoder Simulation Output Lines Per Revolution
--- | ---
Short description | Defines the required lines per revolution when using the encoder simulation mode of Lines Per Rev
Mode | Open‑Loop
Minimum | 1 | Maximum | 16384
Default | 1024 | Units |
Type | 32 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See Encoder Simulation Mode (03.088).

Parameter | 03.093 Encoder Simulation Numerator
--- | ---
Short description | Defines the numerator when using the encoder simulation mode of Ratio
Mode | Open‑Loop
Minimum | 1 | Maximum | 65536
Default | 65536 | Units |
Type | 32 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See Encoder Simulation Mode (03.088).

Parameter | 03.094 Encoder Simulation Denominator
--- | ---
Short description | Defines the denominator when using the encoder simulation mode of Ratio
Mode | Open‑Loop
Minimum | 1 | Maximum | 65536
Default | 65536 | Units |
Type | 32 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See Encoder Simulation Mode (03.088).

Parameter | 03.095 Encoder Simulation Output Roll-over Limit
--- | ---
Short description | Defines the roll-over limit of the output counter and hence the rate at which output markers are produced when using the encoder simulation mode of Ratio
Mode | Open‑Loop
Minimum | 1 | Maximum | 65535
Default | 65535 | Units |
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, BU

See Encoder Simulation Mode (03.088).

Parameter | 03.096 Encoder Simulation SSI Turns Bits
--- | ---
Short description | Defines the number of bits of the outputted SSI data that are used to represent turns information
Mode | Open‑Loop
Minimum | 0 | Maximum | 16
Default | 16 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See Encoder Simulation Mode (03.088).

Parameter | 03.097 Encoder Simulation SSI Comms Bits
--- | ---
Short description | Defines the total number of bits of SSI data to be outputted
Mode | Open‑Loop
Minimum | 2 | Maximum | 48
Default | 33 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See Encoder Simulation Mode (03.088).

Parameter | 03.098 Encoder Simulation Output Mode
--- | ---
Short description | Defines the format of the encoder simulation output
Mode | Open‑Loop
Minimum | 0 | Maximum | 2
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | AB/Gray
1 | FD/Binary
2 | FR/Binary

Encoder Simulation Output Mode (03.098) is used to select the format of the encoder simulation output as given in the table below.

Encoder Simulation Mode (03.088) | Encoder Simulation Output Mode (03.098) | Format
Hardware (0), Lines Per Rev (1), Ratio (2) | AB/Gray | AB quadrature signals
Hardware (0), Lines Per Rev (1), Ratio (2) | FD/Binary | Frequency and direction signals
Hardware (0), Lines Per Rev (1), Ratio (2) | FR/Binary | Forward and reverse signals
SSI (3) | AB/Gray | The position data is in Gray code format. This does not include the “power supply” bit if present.
SSI (3) | FD/Binary, FR/Binary | The position data is in binary format

Parameter | 03.100 F1 Freeze Trigger Source
--- | ---
Short description | Used to select the source that generates trigger events for the F1 system
Mode | Open‑Loop
Minimum | 0 | Maximum | 6
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Digital Input 4
1 | Digital Input 5
2 | P1 Marker
3 | P2 Marker
4 | Common
5 | P1 Zero
6 | P2 Zero

F1 Freeze Trigger Source (03.100) is used to select the source that generates trigger events for the F1 system.

0, 1: Dig I/O 4, Dig I/O 5
Digital I/O 4 or Digital I/O 5 on the drive can be used as trigger sources. If the digital I/O is set up as an input, then trigger events will be produced on the relevant edge of the input signal. If the digital I/O is set up as an output, then trigger events will be produced on the relevant edge of the output signal.

2, 3: Z1, Z2
Z1 selects the P1 position feedback interface marker input as the trigger source and Z2 selects the P2 position feedback interface marker input as the trigger source. No trigger events will be produced unless the selected maker input is available.

4: Common
The output of the common freeze line is selected. If the output of the drive common freeze system is enabled (Bit 3 of Common Freeze Mode (03.112) = 1) then the drive common freeze system provides the freeze event triggers. If the output of the drive common freeze system is disabled the option module freeze line provides the freeze event triggers.

5, 6: P1 Zero, P2 Zero
A freeze event is triggered when the turns for the respective position feedback interface change (i.e. the feedback position passes through zero in either direction). The freeze position stored in F1 Normalised Freeze Position (03.103) or F2 Normalised Freeze Position (03.108) will include the turns associated with the zero position whichever direction the position changes. For example if the turns change from 4 to 5 or 5 to 4 the turns value stored is 5. This mode can be used as a substitute for a physical marker, with a position device that does not have one, to trigger an event to occur at the zero position of the feeback device. For example, it can be used with the AMC to start a CAM at the zero position of the feedback device. It should be noted that if P1 Zero is selected as the trigger source then F1 Freeze Position Source (03.102) has no effect and P1 is always used as the freeze position source. If P2 Zero is selected as the trigger source then F1 Freeze Position Source (03.102) has no effect and P2 is always used as the freeze position source. This is because these freeze trigger sources are only intended to capture the zero position of the device being used to give the zero position trigger event.

Parameter | 03.101 F1 Freeze Mode
--- | ---
Short description | Sets the mode used for the F1 freeze system
Mode | Open‑Loop
Minimum | 0 | Maximum | 3
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Rising 1st
1 | Falling 1st
2 | Rising all
3 | Falling all

0: Rising 1st
Freeze events are produced on the rising edge of the freeze trigger source. If the F1 Freeze Flag (03.104) is 0 then the first suitable edge produced by the trigger source causes the freeze position to be stored and the F1 Freeze Flag (03.104) to be set to 1. No further freeze events are possible until the F1 Freeze Flag (03.104) has been cleared by the user.

1: Falling 1st
As for Rising 1st, but the falling edge is used to trigger freeze events.

2: Rising All
Freeze events are produced on the rising edge of the freeze trigger source. If the F1 Freeze Flag (03.104) is 0 then the first suitable edge produced by the trigger source causes the freeze position to be stored and the F1 Freeze Flag (03.104) to be set to 1. If further suitable edges are produced by the trigger source the freeze position is updated with the current position.

3: Falling All
As for Rising All, but the falling edge is used to trigger freeze events.

Parameter | 03.102 F1 Freeze Position Source
--- | ---
Short description | Defines the source position for the F1 freeze system
Mode | Open‑Loop
Minimum | 0 | Maximum | 2
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | P1
1 | P2
2 | Time

F1 Freeze Position Source (03.102) defines the source for the F1 freeze system as follows:

P1 or P2
When a freeze event occurs, the position from the relevant position feedback interface within the drive (i.e. P1 or P2), including the effect of the marker (see P1 Marker Mode (03.031)), is stored and can be accessed as a 32 bit normalised value in F1 Normalised Freeze Position (03.103). For a digital incremental source (AB, FD, FR, AB Servo, FD Servo or FR Servo) the position is captured at the freeze event using a hardware system. For a resolver the freeze position is the position at the last 250us sample point. For all other position feedback devices the time of the freeze event is captured with hardware and then interpolation, based on the change of position during the previous nominal 250us period, is used to estimate the position at the freeze event.

Time
The time of the freeze event is stored with respect to the last datum used by the position feedback system and option modules fitted to the drive. These datum events occur at a nominal rate of 250us, but if the drive timing is being synchronised by the comms system in an option module then the actual timing may vary slightly depending on the accuracy of the clock providing the sysnchronisation. The time stored in F1 Normalised Freeze Position (03.103) is given as a proportion of the nominal 250us time period where 65536 corresponds to one nomial 250us time period. Note that the value may be positive or negative. Positive values give the time of an event that occured after the last datum, but before the freeze information is processed. Negative values give the time of an event that occurred before the datum, but after the previous time when the freeze information was processed. The time of the freeze event could be used, for example, to determine the value of a virtual position being generated within an option module at the freeze event. The calculated value would only be meaningful if the freeze information is used during the period between the position datum before and after the freeze event, because the time is related to the datum before the freeze information is made available.

Parameter | 03.103 F1 Normalised Freeze Position
--- | ---
Short description | Displays the normalised position from the F1 freeze system
Mode | Open‑Loop
Minimum | -2147483648 | Maximum | 2147483647
Default |  | Units |
Type | 32 Bit Volatile | Update Rate | 250µs write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

See F1 Freeze Position Source (03.102).

Parameter | 03.104 F1 Freeze Flag
--- | ---
Short description | Displays when a freeze event occurs from the F1 freeze system
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | 250µs write
Display Format | Standard | Decimal Places | 0
Coding | RW, ND, NC, PT

The freeze flag is set when a freeze event occurs. If 0 is written to F1 Freeze Flag (03.104) the freeze flag is cleared.

Parameter | 03.105 F2 Freeze Trigger Source
--- | ---
Short description | User to select the source that generates trigger events for the F2 freeze system
Mode | Open‑Loop
Minimum | 0 | Maximum | 6
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Digital Input 4
1 | Digital Input 5
2 | P1 Marker
3 | P2 Marker
4 | Common
5 | P1 Zero
6 | P2 Zero

F2 Freeze Trigger Source (03.105) is used to select the source that generates trigger events for the F2 freeze system.

0, 1: Dig I/O 4, Dig I/O 5
Digital I/O 4 or Digital I/O 5 on the drive can be used as trigger sources. If the digital I/O is set up as an input, then trigger events will be produced on the relevant edge of the input signal. If the digital I/O is set up as an output, then trigger events will be produced on the relevant edge of the output signal.

2, 3: Z1, Z2
Z1 selects the P1 position feedback interface marker input as the trigger source and Z2 selects the P2 position feedback interface marker input as the trigger source. No trigger events will be produced unless the selected maker input is available.

4: Common
The output of the common freeze line is selected. If the output of the drive common freeze system is enabled (Bit 3 of Common Freeze Mode (03.112) = 1) then the drive common freeze system provides the freeze event triggers. If the output of the drive common freeze system is disabled the option module freeze line provides the freeze event triggers.

5, 6: P1 Zero, P2 Zero
A freeze event is triggered when the turns for the respective position feedback interface change (i.e. the feedback position passes through zero in either direction). The freeze position stored in F1 Normalised Freeze Position (03.103) or F2 Normalised Freeze Position (03.108) will include the turns associated with the zero position whichever direction the position changes. For example if the turns change from 4 to 5 or 5 to 4 the turns value stored is 5. This mode can be used as a substitute for a physical marker with a position device that does not have one to trigger an event to occur at the zero position of the feeback device. For example, it can be used with the AMC to start a CAM at the zero position of the feedback device. It should be noted that if P1 Zero is selected as the trigger source then F1 Freeze Position Source (03.102) has no effect and P1 is always used as the freeze position source. If P2 Zero is selected as the trigger source then F1 Freeze Position Source (03.102) has no effect and P2 is always used as the freeze position source. This is because these freeze trigger sources are only intended to capture the zero position of the device being used to give the zero position trigger event.

Parameter | 03.106 F2 Freeze Mode
--- | ---
Short description | Defines the mode for the F2 freeze system
Mode | Open‑Loop
Minimum | 0 | Maximum | 3
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Rising 1st
1 | Falling 1st
2 | Rising all
3 | Falling all

0: Rising 1st
Freeze events are produced on the rising edge of the freeze trigger source. If the F2 Freeze Flag (03.109) is 0 then the first suitable edge produced by the trigger source causes the freeze position to be stored and the F2 Freeze Flag (03.109) to be set to 1. No further freeze events are possible until the F2 Freeze Flag (03.109) has been cleared by the user.

1: Falling 1st
As for Rising 1st, but the falling edge is used to trigger freeze events.

2: Rising All
Freeze events are produced on the rising edge of the freeze trigger source. If the F2 Freeze Flag (03.109) is 0 then the first suitable edge produced by the trigger source causes the freeze position to be stored and the F2 Freeze Flag (03.109) to be set to 1. If further suitable edges are produced by the trigger source the freeze position is updated with the current position.

3: Falling All
As for Rising All, but the falling edge is used to trigger freeze events.

Parameter | 03.107 F2 Freeze Position Source
--- | ---
Short description | Defines the source position for the F2 freeze system
Mode | Open‑Loop
Minimum | 0 | Maximum | 2
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | P1
1 | P2
2 | Time

F2 Freeze Position Source (03.107) defines the source for the F1 freeze system as follows:

P1 or P2
When a freeze event occurs, the position from the relevant position feedback interface within the drive (i.e. P1 or P2), including the effect of the marker (see P1 Marker Mode (03.031)), is stored and can be accessed as a 32 bit normalised value in F2 Normalised Freeze Position (03.108). For a digital incremental source (AB, FD, FR, AB Servo, FD Servo or FR Servo) the position is captured at the freeze event using a hardware system. For a resolver the freeze position is the position at the last 250us sample point. For all other position feedback devices the time of the freeze event is captured with hardware and then interpolation, based on the change of position during the previous nominal 250us period, is used to estimate the position at the freeze event.

Time
The time of the freeze event is stored with respect to the last datum used by the position feedback system and option modules fitted to the drive. These datum events occur at a nominal rate of 250us, but if the drive timing is being synchronised by the comms system in an option module then the actual timing may vary slightly depending on the accuracy of the clock providing the sysnchronisation. The time stored in F2 Normalised Freeze Position (03.108) is given as a proportion of the nominal 250us time period where 65536 corresponds to one nomial 250us time period. Note that the value may be positive or negative. Positive values give the time of an event that occured after the last datum, but before the freeze information is processed. Negative values give the time of an event that occurred before the datum, but after the previous time when the freeze information was processed. The time of the freeze event could be used, for example, to determine the value of a virtual position being generated within an option module at the freeze event. The calculated value would only be meaningful if the freeze information is used during the period between the position datum before and after the freeze event, because the time is related to the datum before the freeze information is made available.

Parameter | 03.108 F2 Normalised Freeze Position
--- | ---
Short description | Displays the normalised position from the F2 freeze system
Mode | Open‑Loop
Minimum | -2147483648 | Maximum | 2147483647
Default |  | Units |
Type | 32 Bit Volatile | Update Rate | 250µs write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

See F2 Freeze Position Source (03.107).

Parameter | 03.109 F2 Freeze Flag
--- | ---
Short description | Displays when a freeze event occurs from the F2 freeze system
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | 250µs write
Display Format | Standard | Decimal Places | 0
Coding | RW, ND, NC, PT

The freeze flag is set when a freeze event occurs. If 0 is written to F2 Freeze Flag (03.109) the freeze flag is cleared.

Parameter | 03.110 Common Freeze Source 1
--- | ---
Short description | Defines source 1 for the common freeze system
Mode | Open‑Loop
Minimum | 0 | Maximum | 4
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Digital Input 4
1 | Digital Input 5
2 | P1 Marker
3 | P2 Marker
4 | Disabled

See F1 Freeze Trigger Source (03.100) or F2 Freeze Trigger Source (03.105). It should be noted that if the Disabled option is selected then the input is set to a one.

Parameter | 03.111 Common Freeze Source 2
--- | ---
Short description | Defines source 2 for the common freeze system
Mode | Open‑Loop
Minimum | 0 | Maximum | 4
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Digital Input 4
1 | Digital Input 5
2 | P1 Marker
3 | P2 Marker
4 | Disabled

See F1 Freeze Trigger Source (03.100) or F2 Freeze Trigger Source (03.105). It should be noted that if the Disabled option is selected then the input is set to a one.

Parameter | 03.112 Common Freeze Mode
--- | ---
Short description | Defines the mode used for the common freeze system
Mode | Open‑Loop
Minimum | 0 (Display: 0000) | Maximum | 15 (Display: 1111)
Default | 0 (Display: 0000) | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Binary | Decimal Places | 0
Coding | RW

The common freeze system can be used to logically combine two freeze trigger sources. The switches in the common freeze system are controlled by the bits in Common Freeze Mode (03.112) as defined in the table below.

Bit | Function
0 | Source 1 input invert 1
1 | Source 2 input invert
2 | Output invert
3 | Output enable

Therefore the value defined bits 2 to 0 can be used to generate various logic functions as given in the table below.

Bits 2 to 0 | Function
0 | Source1 AND Source2
1 | NOT(Source1) AND Source2
2 | Source1 AND NOT(Source2)
3 | Source1 NOR Source2
4 | Source1 NAND Source2
5 | NOT(Source1) NAND Source2
6 | Source1 NAND NOT(Source2)
7 | Source1 OR Source2

Parameter | 03.113 Freeze Input States
--- | ---
Short description | Displays the level of the selected freeze inputs
Mode | Open‑Loop
Minimum | 0 (Display: 00) | Maximum | 3 (Display: 11)
Default |  | Units |
Type | 8 Bit Volatile | Update Rate | 4ms write
Display Format | Binary | Decimal Places | 0
Coding | RO, ND, NC, PT

The bits in Freeze Input States (03.113) show the level of the selected freeze trigger inputs. Bit 0 corresponds to F1 freeze input and bit 1 corresponds to F2 freeze input. It should be noted that if the trigger option is P1Zero or P2Zero there is no hardware trigger input, and so the relevant bit is always zero.

Parameter | 03.118 P1 Thermistor Type
--- | ---
Short description | Defines the thermistor type for the P1 interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 3
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | DIN44082
1 | KTY84
2 | 0.8mA
3 | Encoder

P1 Thermistor Type (03.118) defines the operating mode of the P1 thermistor input.

P1 Thermistor Type (03.118) | Compatible devices
0: DIN44082 | Three thermistors in series as specified in DIN44082 standard
1: KTY84 | KTY84 PTC thermistor
2: 0.8mA | Any device
3: Encoder | EnDat 2.2 encoder

All except 3(Encoder)
If a device is connected between the pin 15 of the encoder interface and 0V a current source will pass 0.8mA through the device with a maximum voltage of approximately 3.8V (i.e. maximum resistance of approximately 4750 Ohms). The resistance of the device is calculated and displayed in P1 Thermistor Feedback (03.119). If P1 Thermistor Type (03.118) is set to select KTY84 the temperature is also calculated and written to P1 Thermistor Temperature (03.122). Note that DIN44082 mode and 0.8mA mode operate in exactly the same way.

3 (Encoder)
If an EnDat 2.2 encoder which supports external temperature feedback is connected to the P1 position feedback interface then it is possible to obtain the measured temperature from the encoder if P1 Thermistor Type (03.118) is set to 3. The temperature is displayed in P1 Thermistor Temperature (03.122) and a resistance equivalent to that for a KTY84 device is displayed in P1 Thermistor Feedback (03.119). The drive does not check if an external device is connected, but short circuit protection can be selected to detect if the device is not connected because the resistance will appear as zero.

Parameter | 03.119 P1 Thermistor Feedback
--- | ---
Short description | Displays the resistance of the thermistor on the P1 interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 5000
Default |  | Units | Ω
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

See P1 Thermistor Type (03.118).

Parameter | 03.120 P1 Thermistor Trip Threshold
--- | ---
Short description | Defines the thermistor trip threshold for the P1 interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 5000
Default | 3300 | Units | Ω
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See P1 Thermistor Fault Detection (03.123).

Parameter | 03.121 P1 Thermistor Reset Threshold
--- | ---
Short description | Defines the thermistor reset threshold for the P1 interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 5000
Default | 1800 | Units | Ω
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See P1 Thermistor Fault Detection (03.123).

Parameter | 03.122 P1 Thermistor Temperature
--- | ---
Short description | Displays the temperature of the device based on the resistance to temperature characteristic for the specified device
Mode | Open‑Loop
Minimum | -50 | Maximum | 300
Default |  | Units | °C
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

See P1 Thermistor Type (03.118).

Parameter | 03.123 P1 Thermistor Fault Detection
--- | ---
Short description | Defines the fault detection for the P1 thermsitor input
Mode | Open‑Loop
Minimum | 0 | Maximum | 2
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | None
1 | Temperature
2 | Temp or Short

Defines the fault detection for the P1 thermsitor input:

P1 Thermistor Fault Detection (03.123) | Fault detection
0: None | No detection active
1: Temperature | Over temperature detection
2: Temp and short | Over temperature and short circuit detection

If over temperature detection is enabled a Thermistor.001 trip is initiated if P1 Thermistor Feedback (03.119) is above the level defined by P1 Thermistor Trip Threshold (03.120). The trip cannot be reset until P1 Thermistor Feedback (03.119) is below P1 Thermistor Reset Threshold (03.121).

If short circuit detection is enabled then a Th Short Circuit.001 is initiated if P1 Thermistor Feedback (03.119) is below 50 Ohms.

Parameter | 03.127 P2 Speed Feedback
--- | ---
Short description | Displays the speed feedback from the P2 interface
Mode | Open‑Loop
Minimum | −VM_SPEED | Maximum | VM_SPEED
Default |  | Units |
Type | 32 Bit Volatile | Update Rate | 4ms write
Display Format | Standard | Decimal Places | 1
Coding | RO, FI, VM, ND, NC, PT

Provided the set-up parameters for the position feedback device connected to the drive P2 position interface are correct P2 Speed Feedback (03.127) shows the speed derived from the feedback. The speed is given in mm/s if P2 Linear Feedback Select (03.151) = 1 and Linear Speed Select (01.055) = 1, otherwise it is given in rpm. The value shown is measured over a 16ms sliding window period, and so the ripple in this value is as defined for Speed Feedback (03.002).

Parameter | 03.128 P2 Revolution/Pole Pitch Counter
--- | ---
Short description | Displays the revolution/pole pitch counter from the P2 interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 65535
Default |  | Units |
Type | 16 Bit Power Down Save | Update Rate | 4ms write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

P2 Revolution/Pole Pitch Counter (03.128), P2 Position (03.129) and P2 Fine Position (03.130) combined give the encoder position with a resolution of 1/232 of a revolution/pole pitch as a 48 bit number. If a rotary position feedback device is being used (P2 Linear Feedback Select (03.151) = 0) then these quantities relate directly to the rotary position of the feedback device. If a linear feedback device is used then one revolution or pole pitch relates to the distance given by P2 Pole Pitch (03.155).

See P1 Revolution/Pole Pitch Counter (03.028) for more information.

Parameter | 03.129 P2 Position
--- | ---
Short description | Displays the position feedback from the P2 interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 65535
Default |  | Units |
Type | 16 Bit Power Down Save | Update Rate | 4ms write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

See P2 Revolution/Pole Pitch Counter (03.128).

Parameter | 03.130 P2 Fine Position
--- | ---
Short description | Displays the fine position from the P2 interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 65535
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | 4ms write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

See P2 Revolution/Pole Pitch Counter (03.128).

Parameter | 03.131 P2 Marker Mode
--- | ---
Short description | Defines the marker mode for the P2 interface
Mode | Open‑Loop
Minimum | 0 (Display: 0000) | Maximum | 15 (Display: 1111)
Default | 4 (Display: 0100) | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Binary | Decimal Places | 0
Coding | RW

P2 Device type (03.138): AB, FD, FR
Each position feedback device produces incremental signals which are counted in hardware. If P2 Marker Mode (03.131) = 0 the following occurs when a marker event is produced by the Z1 input:

1. P2 Position (03.129) and P2 Fine Position (03.130) are reset to zero.
2. The bits in P2 Normalised Position (03.158) related to P2 Position (03.129) and P2 Fine Position (03.130) are reset to zero
3. P2 Marker Flag (03.132) is set to one.

The marker is a hardware function, and so the position appears as though it is reset at the marker event time even if this is between control system sample points. It should be noted that the marker event occurs on the rising edge of the marker pulse if the position change over the last sample was positive or on the falling edge if the position change over the last sample was negative. This ensures that the marker event occurs at the same physical location for either direction of rotation.

The action taken when a marker event occurs can be modified by setting the bits of P2 Marker Mode (03.131) as described in the table below.

Bit | Effect of setting bit to one
0 | No action is taken unless the marker flag is zero before the marker event occurs
1 | P2 Revolution/Pole Pitch Counter (03.128) and the whole of P2 Normalised Position (03.158) are also set to zero on a marker event
2 | P2 Revolution/Pole Pitch Counter (03.128), P2 Position (03.129), P2 Fine Position (03.130) and the related part of P2 Normalised Position (03.158) are not reset. (This overrides bit 1.) P2 Normalised Position (03.158) is transferred to P2 Normalised Marker Position (03.159) and P2 Marker Flag (03.132) is set to one.
3 | This bit in has not effect.

The marker input can be used for a standard type marker function or alternatively it can be used as an additional freeze input for the P1 position feedback interface.

P2 Device type (03.138): Any other device type
The marker function cannot be used and P2 Marker Mode (03.131) has no effect.

Parameter | 03.132 P2 Marker Flag
--- | ---
Short description | Indicates when a marker event occurs
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit Volatile | Update Rate | 250µs write
Display Format | Standard | Decimal Places | 0
Coding | RW, NC

P2 Marker Flag (03.132) is set to one when a marker event occurs. The flag must be cleared by the user.

Parameter | 03.133 P2 Rotary Turns Bits
--- | ---
Short description | Defines the number of rotary turns bit for the P2 interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 16
Default | 16 | Units |
Type | 8 Bit User Save | Update Rate | Background read, auto-configuration write
Display Format | Standard | Decimal Places | 0
Coding | RW

P2 Rotary Turns Bits (03.133) only has any effect if the position feedback interface is being used with a rotary device (i.e. P2 Linear Feedback Select (03.151) = 0).

P2 Device type (03.138): EnDat, BISS, SSI
P2 Rotary Turns Bits (03.133) is used to determine the number of bits within the comms messages from the position feedback device that represent turns. For a single turn encoder P2 Rotary Turns Bits (03.133) must be set to zero. It should be noted that some SSI encoders include leading zeros before the turns information and in this case the number of turns bits should include the leading zeros. The most significant bits in P1 Revolution/Pole Pitch Counter (03.028) that are not included in the turns information provided by the encoder comms are held at zero. If P2 Rotary Turns Bits (03.133) = 0 (single turn encoder) the whole of P2 Revolution/Pole Pitch Counter (03.128) is held at zero.

P2 Device type (03.138): Any other device type
It is sometimes desirable to mask off the most significant bits of P2 Revolution/Pole Pitch Counter (03.128), but this does not have to be done for the drive to function correctly. If P2 Rotary Turns Bits (03.133) = 0 the whole of P2 Revolution/Pole Pitch Counter (03.128) is held at zero. If P2 Rotary Turns Bits (03.133) has any other value it indicates the number of bits in P2 Revolution/Pole Pitch Counter (03.128) that are not held at zero. For example, if P2 Rotary Turns Bits (03.133) = 5, then P2 Revolution/Pole Pitch Counter (03.128) counts up to 31 before being reset.

Parameter | 03.134 P2 Rotary Lines Per Revolution
--- | ---
Short description | Defines the number of rotary lines per revolution for the P2 interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 100000
Default | 1024 | Units |
Type | 32 Bit User Save | Update Rate | Background read, auto-configuration write
Display Format | Standard | Decimal Places | 0
Coding | RW

P2 Rotary Lines Per Revolution (03.134) only has any effect if the position feedback interface is being used with a rotary device (i.e. P2 Linear Feedback Select (03.151) = 0).

P2 Device type (03.138): AB
P2 Rotary Lines Per Revolution (03.134) should be set to the number of lines per revolution for the encoder connected to the P1 position feedback interface.

P2 Device type (03.138): FD, FR
P2 Rotary Lines Per Revolution (03.134) should be set to the number of lines per revolution for the encoder connected to the P1 position feedback interface multiplied by 2.

P2 Device type (03.138): Any other device type
P2 Rotary Lines Per Revolution (03.134) has no effect.

Parameter | 03.135 P2 Comms Bits
--- | ---
Short description | Defines the total number of bits of position information in the comms message from the encoder on the P2 interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 48
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read, auto-configuration write
Display Format | Standard | Decimal Places | 0
Coding | RW

P2 Device type (03.138): EnDat, SSI, BiSS
P2 Comms Bits (03.135) should be set to the total number of bits of position information in the comms message from the encoder. If SSI communications is being used this should include any leading or trailing zeros and the power supply alarm bit if present.

P2 Device type (03.138): Any other device type
P2 Comms Bits (03.135) has no effect.

Parameter | 03.137 P2 Comms Baud Rate
--- | ---
Short description | Defines the baud rate used for encoder communications
Mode | Open‑Loop
Minimum | 0 | Maximum | 8
Default | 2 | Units | Baud
Type | 8 Bit User Save | Update Rate | Background read, auto-configuration write
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | 100k
1 | 200k
2 | 300k
3 | 400k
4 | 500k
5 | 1M
6 | 1.5M
7 | 2M
8 | 4M

P2 Comms Baud Rate (03.137) defines the baud rate used for encoder communications. Restrictions are applied to the baud rate for different feedback devices, and so the baud rate may be different to the parameter value.

P2 Device type (03.138): EnDat, BiSS, SSI
Any baud rate that is within the range specified for the encoder may be used. The line delay is measured during initialisation, and used to compensate this delay during communications with the encoder. Therefore there is no timing based restriction on the length of the cable between the position feedback interface and the encoder. However, care should be taken to ensure that the wiring arrangement and the type of cable used are suitable for the selected baud rate and the distance between the position interface and the encoder. See P2 Low Speed Update Rate Active (03.163) for more details on timing restrictions related to the drive sample times.

P2 Device type (03.138): Any other device
P2 Comms Baud Rate (03.137) has no effect.

Parameter | 03.138 P2 Device type
--- | ---
Short description | Set this to the feedback device type connected to the P2 position interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 6
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | None
1 | AB
2 | FD
3 | FR
4 | EnDat
5 | SSI
6 | BiSS

If P2 Device type (03.138) = Disabled, the P2 position feedback interface is disabled and does not provide any position feedback.

See P1 Device Type (03.038) for more information on the different position feedback device types.

Parameter | 03.140 P2 Error Detection Level
--- | ---
Short description | Used to enable or disable position feedback trip functions
Mode | Open‑Loop
Minimum | 0 (Display: 00000) | Maximum | 31 (Display: 11111)
Default | 1 (Display: 00001) | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Binary | Decimal Places | 0
Coding | RW

This parameter can be used to enable or disable position feedback trip functions as follows:

Bit | Function
0 | Not used with the P2 position interface.
1 | Not used with the P2 position interface.
2 | Enable SSI power supply alarm bit monitor (indicated by trip Encoder 6).
3 | Disable trips Encoder 1 to Encoder 6.
4 | Disable trip Encoder 7.

Bits 3 and 4 do not prevent the device from becoming un-initialised. The trip is suppressed, but the device is still un-initialised and this is indicated by the appropriate bit for the position feedback interface in Position Feedback Initialized (03.076).

Encoder trips
The following table shows trips that can be initiated that are related to the position feedback interface P2. The sub-trip number is 2 for the drive P2 position feedback interface.

Drive trip | Encoders | Reason for error
Encoder 4 | EnDat, BISS | Comms timeout
Encoder 5 | EnDat, BISS | Checksum/CRC error
SSI | Not ready at start of position transfer (i.e. data input not one)
Encoder 6 | EnDat, BiSS | The encoder has indicated an error
SSI | Power supply alarm bit active
Encoder 7 | EnDat, BiSS, SSI | An attempt has been made to enable the drive, but a position feedback device is not initialised
Encoder 8 | EnDat, SSI, BiSS | Maximum Switching Frequency (05.018), P2 Device type (03.138), P2 Comms Bits (03.135), P2 Comms Baud Rate (03.137), P2 Calculation Time (03.160), P2 Recovery Time (03.161), P2 Line Delay Time (03.162) and P2 User Comms Enable (03.167) are used to determine the time taken for the communications exchange with the encoder. If this time exceeds 250μs an Encoder 8 trip is initiated.
Encoder 9 | All | Speed feedback selected from an option slot that does not have a position feedback category option module fitted
Phasing Error | All | Incorrect encoder phasing 1
Encoder 12 | BiSS | The encoder could not be identified during auto-configuration

1. Incorrect encoder phasing is detected if the motor reaches half of the speed defined by VM_SPEED_FREQ_REF[MAX] and the phasing error is large enough for the motor to accelerate uncontrollably.

Wire-break detection
It may be important to detect a break in the connections between the drive and the position feedback device. This feature is provided for most position feedback devices either directly or indirectly as listed below.

Device | Detection method | Trip produced
AB, FD, FR | There is no wire break detection of the A2, B2, and Z2 signals on the P2 position interface. | None
EnDat, BiSS | Wire break in the comms link is detected by a CRC or timeout error. | Encoder 4, Encoder 5
SSI | Wire break detection in the comms is difficult with these devices. However, if power supply alaram bit monitoring is enabled the drive will be looking for a one at the start of the message and a zero to indicate that the power supply is okay. If the clock stops or the data line is disconnected the data input to the drive may stay in one state or the other and cause a trip. | Encoder 5, Encoder 6

Parameter | 03.141 P2 Auto-configuration Select
--- | ---
Short description | Set this parameter to enable auto-configuration of EnDat and BiSS feedback devices
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 1 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Disabled
1 | Enabled

P2 Device type (03.138): EnDat, BiSS
If auto-configuration has not been disabled (i.e. P2 Auto-configuration Select (03.141) = 0) then during position feedback initialisation the encoder is interrogated to determine whether the encoder is a rotary or linear encoder and P2 Linear Feedback Select (03.151) is set up appropriately. Then the following parameters are set up based on information from the encoder:

Rotary | Linear
P2 Rotary Turns Bits (03.133) | P2 Linear Comms Pitch (03.152)
P2 Rotary Lines Per Revolution (03.134) | P2 Linear Line Pitch (03.153)
P2 Comms Bits (03.135) | P2 Comms Bits (03.135)
| P2 Linear Comms And Line Pitch Units (03.154)

The following actions are also taken to set up the timing for the encoder.

Comms Protocol | Actions taken
EnDat 2.1 | P2 Calculation Time (03.160) = From the encoder P2 Recovery Time (03.161) = 30μs Line delay measured and result written to P2 Line Delay Time (03.162)
EnDat 2.2 | P2 Calculation Time (03.160) = From the encoder P2 Recovery Time (03.161) = 4μs and the recovery time within the encoder is set up to the shortest value of 3.75μs if the P2 Comms Baud Rate (03.137) is 1M or more.Line delay measured and result written to P2 Line Delay Time (03.162)
BiSS | P2 Recovery Time (03.161) = 12μs Line delay measured and result written to P2 Line Delay Time (03.162)
SSI | Line delay measured and result written to P2 Line Delay Time (03.162)

If P2 Auto-configuration Select (03.141) = 1 then P2 Comms Baud Rate (03.137) is set to the minimum value that will give a total message transfer time of less than 62μs, so that the transfer will occur at the fast update rate with the minimum baud rate. It should be noted that the value of P2 User Comms Enable (03.167) is taken into account as this may affect the message time.

Once these parameters have been set up it should be possible for the drive to operate correctly with the encoder. The drive repeatedly attempts to initialise the encoder, including auto-configuration which is part of this process, until it is successful. Therefore if auto-configuration has not been successful by the time the drive is enabled because the drive cannot establish communications an Encoder 7 trip occurs. For BiSS encoders the drive must identify the encoder model number to perform auto-configuration. If communications is established, but the drive cannot recognise the encoder model an Encoder 12 trip is produced immediately.

If auto-configuration is disabled (i.e. P2 Auto-configuration Select (03.141) = 1) then none of the above actions are carried out except for the line delay measurement.

P2 Device type (03.138): All other device types
P2 Auto-configuration Select (03.141) has no effect.

Parameter | 03.142 P2 Feedback Filter
--- | ---
Short description | Defines the time period for a sliding window filter that may be applied to the feedback taken from the P2 interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 5
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Disabled
1 | 1ms
2 | 2ms
3 | 4ms
4 | 8ms
5 | 16ms

P2 Feedback Filter (03.142) defines the time period for a sliding window filter that may be applied to the feedback taken from the drive P2 position feedback interface. This is particularly useful in applications where the drive encoder is used to give speed feedback for the speed controller and where the load includes a high inertia, and so the speed controller gains are very high. Under these conditions, without a filter on the feedback, it is possible for the speed loop output to change constantly from one current limit to the other and lock the integral term of the speed controller.

Parameter | 03.143 P2 Maximum Reference
--- | ---
Short description | Defines the maximum speed reference from the P2 interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 35940
Default | 1500 | Units |
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, BU

The speed feedback from the drive P1 position feedback interface can be used as a source to control a parameter. The speed feedback is scaled to give a value as a percentage of P2 Maximum Reference (03.143) in 0.1% units which is displayed in P2 Reference (03.145). The value is then scaled by the P2 Reference Scaling (03.144) and then routed to the destination defined by P2 Reference Destination (03.146).

Normally the destination is updated every 4ms, but if the destination is the Hard Speed Reference (03.022), P2 Maximum Reference (03.143) = VM_SPEED_FREQ_REF[MAX] and P2 Reference Scaling (03.144) = 1.000 it is updated every 250μs. Although the hard speed reference is updated every 250μs internally a value in rpm or mm/s is written to Hard Speed Reference (03.022) every 4ms for indication only. It should be noted that if the fast update method is used the resolution of the speed feedback devived from the position feedback device defines the resolution of the hard speed reference and that any ripple on the feedback will be present on the hard speed reference (see Speed Feedback (03.002)).

Parameter | 03.144 P2 Reference Scaling
--- | ---
Short description | Defines the scaling applied to the P2 reference
Mode | Open‑Loop
Minimum | 0.000 | Maximum | 4.000
Default | 1.000 | Units |
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 3
Coding | RW

See P2 Maximum Reference (03.143).

Parameter | 03.145 P2 Reference
--- | ---
Short description | Displays the value in P2 reference
Mode | Open‑Loop
Minimum | -100.0 | Maximum | 100.0
Default |  | Units | %
Type | 16 Bit Volatile | Update Rate | 4ms write
Display Format | Standard | Decimal Places | 1
Coding | RO, FI, ND, NC, PT

See P2 Maximum Reference (03.143).

Parameter | 03.146 P2 Reference Destination
--- | ---
Short description | Defines the destination parameter for P2 reference
Mode | Open‑Loop
Minimum | 0.000 | Maximum | 59.999
Default | 0.000 | Units |
Type | 16 Bit User Save | Update Rate | Drive reset read
Display Format | Standard | Decimal Places | 3
Coding | RW, DE, PT, BU

See P2 Maximum Reference (03.143).

Parameter | 03.147 P2 SSI Incremental Mode
--- | ---
Short description | Set to 1 to enable SSI incremental mode
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

P2 Device type (03.138): SSI
If P2 SSI Incremental Mode (03.147) = 0 the complete absolute position is read at each sample. Care should be taken when using this mode as some unwanted effects can occur when the encoder passes through the boundary between its maximum position and zero. In this mode the encoder can be used for motor control provided at least 6 bits of turns information are provided by the encoder otherwise an over speed trip will be produced as the position passes over the maximum position to zero boundary. P2 Normalised Position (03.158) can be used for position control over this boundary provided the normalised turns bits are set up so that the normalised positions do not contain turns information that is not available from the encoder. As the SSI format does not include any error checking it is not possible to detect if the position data has been corrupted by noise. The benefit of using the absolute position directly from an SSI encoder is that even if the encoder communications are disturbed by noise and position errors occur, the position will always recover the correct position after the disturbance has ended.

If P2 SSI Incremental Mode (03.147) = 1 the absolute position is only taken from the encoder during initialisation. The change of position over each sample is then accumulated to determine the position. This method always gives 16 bits of turns information that can always be used without jumps in position whatever value is used as the turns bits for normalisation. If noise corrupts the data from an SSI encoder it is possible to have apparent large change of position, and this can result in the turns information becoming and remaining corrupted until the encoder is re-initialised.

If an SSI encoder is used, but is not powered from the drive, and the encoder is powered up after the drive, it is possible that the first change of position detected could be large enough to cause the problems described above. This can be avoided if the encoder interface is initialised with Initialise Position Feedback (03.075) after the encoder has powered up. If the encoder includes a power supply alarm bit, the power supply monitor should be enabled. This will ensure that the drive remains tripped until the encoder is powered up and the action of resetting the trip will reinitialise the encoder interface.

P2 Device type (03.138): All other device types
P2 SSI Incremental Mode (03.147) has no effect.

Parameter | 03.148 P2 SSI Binary Mode
--- | ---
Short description | Set to 1 to enable SSI binary mode
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

P2 Device type (03.138): SSI
SSI encoders normally use Gray code data format. However, some encoders use binary format which may be selected by setting P2 SSI Binary Mode (03.148) to one.

P2 Device type (03.138): All other device types
P2 SSI Binary Mode (03.148) has no effect.

Parameter | 03.149 P2 Additional Power-up Delay
--- | ---
Short description | Defines an additional delay for when any attempt is made to communicate to the device P2
Mode | Open‑Loop
Minimum | 0.0 | Maximum | 25.0
Default | 0.0 | Units | s
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 1
Coding | RW, BU

When the position feedback is initialised, at power-up or at any other time, a delay is included before the information from the feedback device is used or any attempt is made to communicate with the device. P2 Additional Power-up Delay (03.149) defines an additional delay that is added to the minimum delay. See P1 Additional Power-up Delay (03.049) for the minimum delays for the different position feedback device types.

Parameter | 03.150 P2 Feedback Lock
--- | ---
Short description | Set to 1 to prevent the position feedback paramters for P2 being updated
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

If P2 Feedback Lock (03.150) = 1 then P2 Revolution/Pole Pitch Counter (03.128), P2 Position (03.129) and P2 Fine Position (03.130) are not updated. If P2 Feedback Lock (03.150) = 0 then these parameters are updated normally.

Parameter | 03.151 P2 Linear Feedback Select
--- | ---
Short description | Set to 1 to configure the P2 interface to operate with a linear position feedback device
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read, auto-configuration write
Display Format | Standard | Decimal Places | 0
Coding | RW

If P2 Linear Feedback Select (03.151) = 0 then the drive P1 position feedback interface is configured to operate with a rotary position feedback device. P2 Rotary Turns Bits (03.133) and P2 Rotary Lines Per Revolution (03.134) should be used to set up the position feedback interface.

If P2 Linear Feedback Select (03.151) = 1 then the position feedback interface is configured to operate with a linear position feedback device. P2 Linear Comms Pitch (03.152) and P2 Linear Line Pitch (03.153) should be used to set up the position feedback interface.

Parameter | 03.152 P2 Linear Comms Pitch
--- | ---
Short description | Defines the distance covered by the least significant bit of the position information in a comms message from a linear encoder
Mode | Open‑Loop
Minimum | 0.001 | Maximum | 100.000
Default | 0.001 | Units |
Type | 32 Bit User Save | Update Rate | Background read, auto-configuration write
Display Format | Standard | Decimal Places | 3
Coding | RW

P2 Device type (03.138): EnDat, SSI, BiSS
P2 Linear Comms Pitch (03.152) is used to define the distance covered by the least significant bit of the position information in a comms message from a linear encoder. The units used by this parameter are defined by P2 Linear Comms And Line Pitch Units (03.154).

P2 Device type (03.138): Any other device
P2 Linear Comms Pitch (03.152) has no effect.

Parameter | 03.153 P2 Linear Line Pitch
--- | ---
Short description | Defines the linear line pitch for device P2
Mode | Open‑Loop
Minimum | 0.001 | Maximum | 100.000
Default | 0.001 | Units |
Type | 32 Bit User Save | Update Rate | Background read, auto-configuration write
Display Format | Standard | Decimal Places | 3
Coding | RW

P2 Linear Line Pitch (03.153) only has any effect if the position feedback interface is being used with a linear device (i.e. P2 Linear Feedback Select (03.151) = 1) and should be used to define the distances listed below for each type of device. The units used by this parameter are defined by P2 Linear Comms And Line Pitch Units (03.154).

P2 Device type (03.138): AB
P2 Linear Line Pitch (03.153) should be set to the distance covered by one line period on the encoder.

P2 Device type (03.138): FD, FR
P2 Linear Line Pitch (03.153) should be set to the distance covered by two line periods on the encoder.

P2 Device type (03.138): Any other device
P2 Linear Line Pitch (03.153) has no effect.

Parameter | 03.154 P2 Linear Comms And Line Pitch Units
--- | ---
Short description | Defines the linear units in either millimetres or micrometres
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | millimetres
1 | micrometres

P2 Linear Comms And Line Pitch Units (03.154) defines the units used by P2 Linear Comms Pitch (03.152) and P2 Linear Line Pitch (03.153) in millimetres or micrometres.

Parameter | 03.155 P2 Pole Pitch
--- | ---
Short description | Defines the distance equivalent to one pole for linear position feedback devices
Mode | Open‑Loop
Minimum | 0.01 | Maximum | 1000.00
Default | 10.00 | Units | mm
Type | 32 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

P2 Pole Pitch (03.155) is used to define the distance equivalent to one pole for linear position feedback devices. If the linear position feedback device is being used with a linear motor, then P2 Pole Pitch (03.155) should be set to the pole pitch of the motor.

Parameter | 03.156 P2 Feedback Reverse
--- | ---
Short description | Set to 1 to reverse the direction of the position feedback
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

If P2 Feedback Reverse (03.156) = 1 the position feedback is negated. This can be used to reverse the direction of the position feedback.

Parameter | 03.157 P2 Normalisation Turns
--- | ---
Short description | Defines the number of turns bits included in the normalisation parameters
Mode | Open‑Loop
Minimum | 0 | Maximum | 16
Default | 16 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

P2 Normalisation Turns (03.157) defines the number of turns bits included in the following parameters. See P1 Normalisation Turns (03.057) for more information.

P2 Normalised Position (03.158)
P2 Normalised Marker Position (03.159)
F1 Normalised Freeze Position (03.103) if P2 is the source position for freeze function F1
F2 Normalised Freeze Position (03.108) if P2 is the source position for freeze function F2

Parameter | 03.158 P2 Normalised Position
--- | ---
Short description | Displays the position taken from the position feedback device including the effect of the marker function
Mode | Open‑Loop
Minimum | -2147483648 | Maximum | 2147483647
Default |  | Units |
Type | 32 Bit Volatile | Update Rate | 250µs write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

P2 Normalised Position (03.158) is the position taken from the position feedback device including the effect of the marker function. See P2 Normalisation Turns (03.157) for details of the format.

Parameter | 03.159 P2 Normalised Marker Position
--- | ---
Short description | Displays the normalised position at the last marker event
Mode | Open‑Loop
Minimum | -2147483648 | Maximum | 2147483647
Default |  | Units |
Type | 32 Bit Volatile | Update Rate | 250µs write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

P2 Normalised Marker Position (03.159) is the value P2 Normalised Position (03.158) at the last marker event provided bit 2 of P2 Marker Mode (03.131) is set to 1. See P2 Marker Mode (03.131) for more details.

Parameter | 03.160 P2 Calculation Time
--- | ---
Short description | Defines the time from the first edge of the clock signal from the position feedback interface until the encoder has calculated the position and is ready to return this information
Mode | Open‑Loop
Minimum | 0 | Maximum | 20
Default | 5 | Units | µs
Type | 8 Bit User Save | Update Rate | Background read, auto-configuration write
Display Format | Standard | Decimal Places | 0
Coding | RW

P2 Device type (03.138): EnDat
P2 Calculation Time (03.160) is the time from the first edge of the clock signal from the position feedback interface until the encoder has calculated the position and is ready to return this information. This is used to calculate the overall time for a message interchange with the encoder. See P2 Low Speed Update Rate Active (03.163) for more details.

P2 Device type (03.138): Any other type of device
P2 Calculation Time (03.160) has no effect.

Parameter | 03.161 P2 Recovery Time
--- | ---
Short description | Defines the time that must be allowed after each message interchange before a new message begins
Mode | Open‑Loop
Minimum | 4 | Maximum | 100
Default | 30 | Units | µs
Type | 8 Bit User Save | Update Rate | Background read, auto-configuration write
Display Format | Standard | Decimal Places | 0
Coding | RW

P2 Device type (03.138): EnDat, SSI, BiSS
P2 Recovery Time (03.161) is the time that must be allowed after each message interchange before a new message begins.

P2 Device type (03.138): Any other type of device
P2 Recovery Time (03.161) has no effect.

Parameter | 03.162 P2 Line Delay Time
--- | ---
Short description | Displays the transmission delay between the position feedback interface and the encoder and back again
Mode | Open‑Loop
Minimum | 0 | Maximum | 5000
Default |  | Units | ns
Type | 16 Bit User Save | Update Rate | Background read, position feedback initialisation write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

P2 Device type (03.138): EnDat, SSI, BiSS
During position feedback initialisation the transmission delay between the position feedback interface and the encoder and back again is measured and stored in P2 Line Delay Time (03.162). This value is then used to compensate for this delay so that the clock/data skew does not prevent the data from the encoder from being read. This means that longer line lengths can be used with these feedback devices provided the correct cable and connection arrangements are used.

P2 Device type (03.138): Any other type of device
P2 Line Delay Time (03.162) is always zero.

Parameter | 03.163 P2 Low Speed Update Rate Active
--- | ---
Short description | Indicates when the low speed update rate is active
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

P2 Device type (03.138): EnDat, SSI, BISS
If the position can be sampled in 60μs P2 Low Speed Update Rate Active (03.163) = 0, otherwise P2 Low Speed Update Rate Active (03.163) = 1.

The following parameters are used by the drive to determine the necessary time to obtain the required data from the position feedback device.

P2 Rotary Turns Bits (03.133)
P2 Comms Bits (03.135)
P2 Comms Baud Rate (03.137)
P2 Calculation Time (03.160)
P2 Recovery Time (03.161)
P2 Line Delay Time (03.162)
P2 User Comms Enable (03.167)

See P1 Low Speed Update Rate Active (03.063) for more information on how this time is calculated.

P2 Device type (03.138): Any other type of device
P2 Low Speed Update Rate Active (03.163) is always zero.

Parameter | 03.164 P2 Encoder Protocol Detected
--- | ---
Short description | Defines which protocol is used with the device P2
Mode | Open‑Loop
Minimum | 0 | Maximum | 4
Default |  | Units |
Type | 8 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, TE, ND, NC, PT

Value | Text
0 | None
1 | Hiperface
2 | EnDat2.1
3 | EnDat2.2
4 | BiSS

P2 Encoder Protocol Detected (03.164) shows the encoder comms protocol detected during position feedback initialisation. If P2 Device type (03.138) is set to BiSS then P2 Encoder Protocol Detected (03.164) is set to the appropriate value after successful communication with the encoder during initialisation. If P2 Device type (03.138) is set to EnDat then P2 Encoder Protocol Detected (03.164) is set to the appropriate EnDat protocol after successful communication with the encoder during initialisation. If communications is not successful during initialisation then P2 Encoder Protocol Detected (03.164) is set to 0 (None).

Parameter | 03.167 P2 User Comms Enable
--- | ---
Short description | Enables the use of the user comms paramters to communicate to the encoder connected to P2
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 8 Bit Volatile | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

If P2 User Comms Enable (03.167) set to a non-zero value it is possible to use P2 User Comms Transmit Register (03.168) and P2 User Comms Receive Register (03.169) to communicate with an encoder that has a Hiperface, EnDat 2.1, EnDat2.2 or BiSS interface. See P1 User Comms Enable (03.067) for a description of how to use these registers.

Parameter | 03.168 P2 User Comms Transmit Register
--- | ---
Short description | Defines the value present in the user comms transmit register
Mode | Open‑Loop
Minimum | 0 | Maximum | 65535
Default | 0 | Units |
Type | 16 Bit Volatile | Update Rate | Background read/write
Display Format | Standard | Decimal Places | 0
Coding | RW, NC, PT, BU

See P2 User Comms Enable (03.167).

Parameter | 03.169 P2 User Comms Receive Register
--- | ---
Short description | Defines the value present in the user comms receive register
Mode | Open‑Loop
Minimum | 0 | Maximum | 65535
Default | 0 | Units |
Type | 16 Bit Volatile | Update Rate | Background read/write
Display Format | Standard | Decimal Places | 0
Coding | RW, NC, PT, BU

See P2 User Comms Enable (03.167).

Parameter | 03.171 P2 Error Detected
--- | ---
Short description | Indicates if an error has been detected with the position feedback device connected to the P1 position interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

P2 Error Detected (03.171) is set if an error has been detected with the position feedback device connected to the P2 position interface. This parameter is useful if encoder trips have been disabled with P2 Error Detection Level (03.140).

Parameter | 03.172 P2 Status
--- | ---
Short description | Displays the status of the P2 position interface
Mode | Open‑Loop
Minimum | 0 | Maximum | 9
Default |  | Units |
Type | 8 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, TE, ND, NC, PT

Value | Text
0 | None
1 | AB
2 | FD
3 | FR
4 | EnDat
5 | SSI
6 | BiSS
7 | EnDat Alt
8 | SSI Alt
9 | BiSS Alt

Priority of the 15-way D-type is assigned in the following order from the highest priority to the lowest.

1. P1 position interface
2. Encoder simulation output
3. P2 position interface

The availability of the P2 position interface on the 15-way D-type on the drive is dependent on type of feedback device selected in P1 Device Type (03.038) and the encoder simulation mode selected in Encoder Simulation Mode (03.088). P2 Status (03.172) shows the status of the P2 position interface depending on the settings in P2 Device type (03.138), P1 Device Type (03.038), and Encoder Simulation Mode (03.088).

0: None
The P2 position interface is not available.

1: AB
2: FD
3: FR
4: EnDat
5: SSI
6: BiSS
The P2 position interface is available. The connections for the P2 position interface are shown below.

P2 Status (03.172) | 15-way D-type connections
1/2 | 3/4 | 5/6 | 7/8 | 9/10 | 11/12
AB |  |  |  | A2 | B2 | Z2
FD |  |  |  | F2 | D2 | Z2
FR |  |  |  | F2 | R2 | Z2
EnDat |  |  |  | D2 | Clk2 | Z2
SSI |  |  |  | D2 | Clk2 | Z2
BiSS |  |  |  | D2 | Clk2 | Z2

7: EnDat Alt
8: SSI Alt
9: BiSS Alt
The P2 position interface is available but uses alternative connections as shown below as connection 7/8 and 9/10 are used by the encoder simulation output.

P2 Status (03.172) | 15-way D-type connections
1/2 | 3/4 | 5/6 | 7/8 | 9/10 | 11/12
EnDat Alt |  |  | D2 | AOut | BOut | Clk2
SSI Alt |  |  | D2 | AOut | BOut | Clk2
BiSS Alt |  |  | D2 | AOut | BOut | Clk2

See the introduction to this menu for more information on the position feedback interfaces.

Parameter | 03.173 P2 Absolute Turns Recovery Enable
--- | ---
Short description | Set to 1 to allow turns information beyond the number of turns bits provided by the position feedback device connected to P2 to be stored on power-down and recovered at next power-up
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background Read
Display Format | Standard | Decimal Places | 0
Coding | RW

See P1 Absolute Turns Recovery Enable (03.073).

Parameter | 03.174 P2 Additional Configuration
--- | ---
Short description | Provides additional configuration information for the position feedback device not included in the other set-up parameters.
Mode | Open‑Loop
Minimum | 0 | Maximum | 511116116
Default | 0 | Units |
Type | 32 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See P1 Additional Configuration (03.074).