# Menu 10 Single Line Descriptions − Status and Trips

Mode: RFC‑S

Parameter | Range | Default | Type
--- | --- | --- | ---
10.001 | Drive Healthy | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.002 | Drive Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.003 | Zero Speed | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.004 | Running At Or Below Minimum Speed | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.005 | Below Set Speed | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.006 | At Speed | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.007 | Above Set Speed | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.008 | Rated Load Reached | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.009 | Current Limit Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.010 | Regenerating | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.011 | Braking IGBT Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.012 | Braking Resistor Alarm | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.013 | Reverse Direction Commanded | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.014 | Reverse Direction Running | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.015 | Supply Loss | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.016 | Under Voltage Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.017 | Motor Overload Alarm | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.018 | Drive Over‑temperature Alarm | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.019 | Drive Warning | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.020 | Trip 0 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.021 | Trip 1 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.022 | Trip 2 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.023 | Trip 3 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.024 | Trip 4 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.025 | Trip 5 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.026 | Trip 6 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.027 | Trip 7 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.028 | Trip 8 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.029 | Trip 9 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.030 | Braking Resistor Rated Power | 0.000 to 99999.999 kW | 0.000 kW | RW | Num |  |  |  | US
10.031 | Braking Resistor Thermal Time Constant | 0.000 to 1500.000 s | 0.000 s | RW | Num |  |  |  | US
10.032 | External Trip | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
10.033 | Drive Reset | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
10.034 | Number Of Auto‑reset Attempts | None (0), 1 (1), 2 (2), 3 (3), 4 (4), 5 (5), Infinite (6) | None (0) | RW | Txt |  |  |  | US
10.035 | Auto‑reset Delay | 1.0 to 600.0 s | 1.0 s | RW | Num |  |  |  | US
10.036 | Auto‑reset Hold Drive Healthy | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
10.037 | Action On Trip Detection | 00000 to 11111 | 00000 | RW | Bin |  |  |  | US
10.038 | User Trip | 0 to 255 |  | RW | Num | ND | NC |  |
10.039 | Braking Resistor Thermal Accumulator | 0.0 to 100.0 % |  | RO | Num | ND | NC | PT |
10.040 | Status Word | 000000000000000 to 111111111111111 |  | RO | Bin | ND | NC | PT |
10.041 | Trip 0 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.042 | Trip 0 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.043 | Trip 1 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.044 | Trip 1 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.045 | Trip 2 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.046 | Trip 2 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.047 | Trip 3 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.048 | Trip 3 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.049 | Trip 4 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.050 | Trip 4 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.051 | Trip 5 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.052 | Trip 5 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.053 | Trip 6 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.054 | Trip 6 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.055 | Trip 7 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.056 | Trip 7 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.057 | Trip 8 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.058 | Trip 8 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.059 | Trip 9 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.060 | Trip 9 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.061 | Braking Resistor Resistance | 0.00 to 10000.00 Ω | 0.00 Ω | RW | Num |  |  |  | US
10.062 | Low Load Detected Alarm | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.063 | Local Keypad Battery Low | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.064 | Remote Keypad Battery Low | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.065 | Auto‑tune Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.066 | Limit Switch Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.067 | Fire Mode Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.068 | Hold Drive Healthy on Under Voltage | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
10.069 | Additional Status Bits | 0000000000 to 1111111111 |  | RO | Bin | ND | NC | PT |
10.070 | Trip 0 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.071 | Trip 1 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.072 | Trip 2 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.073 | Trip 3 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.074 | Trip 4 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.075 | Trip 5 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.076 | Trip 6 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.077 | Trip 7 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.078 | Trip 8 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.079 | Trip 9 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.080 | Stop Motor | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.081 | Phase Loss | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.101 | Drive Status | Inhibit (0), Ready (1), Stop (2), Scan (3), Run (4), Supply Loss (5), Deceleration (6), dc Injection (7), Position (8), Trip (9), Active (10), Off (11), Hand (12), Auto (13), Heat (14), Under Voltage (15), Phasing (16) |  | RO | Txt | ND | NC | PT |
10.102 | Trip Reset Source | 0 to 1023 |  | RO | Num | ND | NC | PT | PS
10.103 | Trip Time Identifier | -2147483648 to 2147483647 ms |  | RO | Num | ND | NC | PT |
10.104 | Active Alarm | None (0), Brake Resistor (1), Motor Overload (2), Ind Overload (3), Drive Overload (4), Auto Tune (5), Limit Switch (6), Fire Mode (7), Low Load (8), Option Slot 1 (9), Option Slot 2 (10), Option Slot 3 (11), Option Slot 4 (12) |  | RO | Txt | ND | NC | PT |
10.105 | Hand Off Auto State | Not Active (0), Off (1), Hand (2), Auto (3) |  | RO | Txt | ND | NC | PT | PS
10.106 | Potential Drive Damage Conditions | 0000 to 1111 |  | RO | Bin | ND | NC | PT | PS
10.107 | Auto‑tune State | Not Active (0), Resistance (1), pLs (2), Ls (3), Flux (4), Flux Repeat (5), Ld Lq No‑load (6), Lq (7), Ke (8), Inertia (9) |  | RO | Txt | ND | NC | PT |

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |